For 1990-2009 cars

Table 1: | Air Temperature Actuator
Table 2: | A/C Compressor Clutch
Table 3: | A/C Refrigerant Pressure Sensor
Table 4: | Blower Motor
Table 5: | Blower Resistor Assembly
Table 6: | Heater A/C Control Assembly C1
Table 7: | Heater A/C Control Assembly C2

#### Air Temperature Actuator

Connector Part Information |

• | 12064993

• | 6 Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
5-6 | -- | -- | Not Used
7 | BLK/WHT | 251 | Ground-Clean
8 | LT BLU | 733 | Air Temperature Valve Position Sensor Signal
9 | -- | -- | Not Used
10 | BRN | 41 | Fused Output-Ignition 3

#### A/C Compressor Clutch

Connector Part Information |

• | 12162017

• | 2 Way F Metri-Pack 150 Series (MD)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 729 | A/C Compressor Clutch Solenoid Output
B | DK GRN | 59 | A/C Compressor Clutch Solenoid Feed

#### A/C Refrigerant Pressure Sensor

Connector Part Information |

• | 12110192

• | 3 Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2751 | 5-Volt Return
B | GRY | 2700 | 5-Volt Reference
C | RED/BLK | 380 | A/C Refrigerant Pressure Sensor Signal

#### Blower Motor

Connector Part Information |

• | 12064829

• | 2 Way F Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 250 | Ground
B | PPL | 65 | Blower Motor Feed

#### Blower Resistor Assembly

Connector Part Information |

• | 12084890

• | 5 Way F Metri-Pack 280 Series Sealed (MD)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 72 | Blower Switch Output-Medium 2
B | YEL | 60 | Blower Switch Output-Low
C | TAN | 63 | Blower Switch Output-Medium 1
D | PPL | 73 | Blower Switch Output-Medium 3
E | DK BLU | 101 | Blower Resistor Output

#### Heater A/C Control Assembly C1

Connector Part Information |

• | 12064998

• | 8 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BRN | 641 | Fused Output - Ignition 3
C | ORN | 52 | Blower Switch Output-High
D | -- | -- | Not Used
E | PPL | 73 | Blower Switch Output-Medium 3
F | LT BLU | 72 | Blower Switch Output-Medium 2
G | TAN | 63 | Blower Switch Output-Medium 1
H | YEL | 60 | Blower Switch Output-Low

#### Heater A/C Control Assembly C2

Connector Part Information |

• | 12064799

• | 12 Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | LT GRN | 66 | A/C Switch Output
C | BRN | 41 | Fused Output - Ignition 3
D | WHT | 193 | Rear Defogger Relay Output-Coil
E | ORN | 1440 | Fused Output-Battery
F | -- | -- | Not Used
G | LT BLU | 733 | Air Temperature Valve Position Sensor Signal
H | -- | -- | Not Used
J | GRY | 8 | IP Lamp Feed
K | BLK/WHT | 251 | Ground
L | -- | -- | Not Used
M | BRN | 9 | Parklamp Feed