For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | 7x Crankshaft Position (CKP) Sensor
Table 3: | 24x Crankshaft Position (CKP) Sensor
Table 4: | Engine Coolant Temperature (ECT) Sensor
Table 5: | Engine Oil Pressure Sensor
Table 6: | Engine Oil Level Switch
Table 7: | Evaporative Emission (EVAP) Canister Purge Valve
Table 8: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 9: | Exhaust Gas Recirculation (EGR) Valve
Table 10: | Ignition Control Module C1
Table 11: | Ignition Control Module C2
Table 12: | Ignition Control Module C3
Table 13: | Fuel Injectors
Table 14: | Fuel Tank Pressure Sensor
Table 15: | Fuel Tank Module
Table 16: | Pre Converter Heated Oxygen Sensor (HO2S 1)
Table 17: | Post Converter Heated Oxygen Sensor (HO2S 2)
Table 18: | Idle Air Control (IAC) Valve
Table 19: | Intake Air Temperature (IAT) Sensor
Table 20: | Knock Sensor
Table 21: | Manifold Absolute Pressure (MAP) Sensor
Table 22: | Mass Air Flow (MAF) Sensor
Table 23: | Throttle Position (TP) Sensor
Table 24: | Park/Neutral Position Switch C1
Table 25: | Park Neutral Position Switch C2
Table 26: | Vehicle Speed Sensor (VSS)

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/WHT | 812 | Camshaft Position (CMP) Feed (12 Volt Reference)
B | BRN/WHT | 633 | Camshaft Position Sensor Signal
C | BLK | 407 | Camshaft Sensor Position-Low

#### 7x Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Sealed Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
B | PPL | 574 | Crankshaft Position Sensor Signal
A | YEL | 573 | Crankshaft Position Sensor Return

#### 24x Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/WHT | 812 | 12 Volt Reference Feed
B | LT BLU/BLK | 647 | Crankshaft Position Sensor Signal
C | BLK | 407 | Crankshaft Position-Low

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162194

• | 2-Way F Metri-Pack 150.2 Series Sealed P2S (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 452 | Sensor Return
B | YEL | 410 | Coolant Temperature Sensor Signal

#### Engine Oil Pressure Sensor

Connector Part Information |

• | 12065299

• | 1-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 231 | Engine Oil Pressure Switch Signal

#### Engine Oil Level Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 451 | Engine Control Module Ground
B | BRN | 1174 | Oil Level Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Fuse Output-Ignition 3
B | DK GRN/WHT | 428 | EVAP Canister Purge Solenoid Output

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Connector Part Information |

• | 12059863

• | 2-Way F Metri-Pack 150 Series Sealed (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition Feed
B | WHT | 1310 | EVAP Canister Vent Solenoid Output

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 12162826

• | 5-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | Exhaust Gas Recirculation (EGR) Valve Solenoid-LOW
B | BLK | 2753 | Exhaust Gas Recirculation (EGR) Sensor Return
C | BRN/WHT | 1456 | Exhaust Gas Recirculation (EGR) Pintle Position
D | BRN/WHT | 2702 | Exhaust Gas Recirculation (EGR) 5V Reference
E | RED | 1676 | Exhaust Gas Recirculation (EGR) Valve Solenoid-HIGH

#### Ignition Control Module C1

Connector Part Information |

• | 12162261

• | 6-Way F Metri-pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 424 | Electronic Spark Timing Bypass Signal
B | WHT | 423 | Electronic Spark Timing Control Signal
C-D | -- | -- | Not Used
E | PPL/WHT | 430 | Electronic Spark Timing High Reference Signal
F | RED/BLK | 453 | Electronic Spark Timing Low Reference Signal

#### Ignition Control Module C2

Connector Part Information |

• | 12162186

• | 3-Way F Metri-pack 150.1 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 573 | Crankshaft Position Sensor Return
B | -- | -- | Not Used
C | PPL | 574 | Crankshaft Position Sensor Signal

#### Ignition Control Module C3

Connector Part Information |

• | 12162195

• | 2-Way F Metri-pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 450 | Ground
B | PNK | 239 | Ignition Feed

#### Fuel Injectors

Connector Part Information |

• | 12129140

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
Injector 1
A | PNK | 639 | Fuel Injector Feed
B | BLK | 1744 | Fuel Injector #1Output
Injector 2
A | PNK | 639 | Fuel Injector Feed
B | LT GRN/BLK | 1745 | Fuel Injector #2 Output
Injector 3
A | PNK | 639 | Fuel Injector Feed
B | PNK/BLK | 1746 | Fuel Injector #3Output
Injector 4
A | PNK | 639 | Fuel Injector Feed
B | LT BLU/BLK | 844 | Fuel Injector #4Output
Injector 5
A | PNK | 639 | Fuel Injector Feed
B | BLK/WHT | 845 | Fuel Injector #5Output
Injector 6
A | PNK | 639 | Fuel Injector Feed
B | YEL/BLK | 846 | Fuel Injector #6Output

#### Fuel Tank Pressure Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2759 | MAP Sensor Return
B | DK GRN | 890 | Fuel Tank Pressure Signal
C | GRY | 2709 | 5V Sensor Reference

#### Fuel Tank Module

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1589 | Fuel Guage Sensor Signal
B | GRY | 120 | Fuel Pump Motor Feed
C | BLK | 150 | Ground
D | BLK/WHT | 2759 | Fuel Guage Sensor Ground

#### Pre Converter Heated Oxygen Sensor (HO2S 1)

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | Oxygen Sensor Return
B | PPL | 412 | Oxygen Sensor Signal
C | BLK | 250 | Ground
D | BRN | 241 | Ignition Feed

#### Post Converter Heated Oxygen Sensor (HO2S 2)

Connector Part Information |

• | 12160825

• | 4-Way M Metri-pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | Oxygen Sensor Return
B | PPL/WHT | 1668 | Oxygen Sensor Signal
C | BLK | 250 | Ground
D | BRN | 241 | Ignition Feed

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | Idle Air Control (IAC) Valve Motor Feed- Low
B | LT GRN/WHT | 1749 | Idle Air Control (IAC) Valve Motor Feed- High
C | LT BLU/BLK | 1748 | Idle Air Control (IAC) Valve Motor Feed- Low
D | LT BLU/WHT | 1747 | Idle Air Control (IAC) Valve Motor Feed - High

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162199

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | Sensor Return
B | TAN | 472 | Intake Air Temperature (IAT) Sensor Signal

#### Knock Sensor

Connector Part Information |

• | 12176800

• | 1-Way F Metri-Pack 150 Series Sealed (GRAY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 496 | Knock Sensor Signal 1

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12020403

• | 3-Way M WeatherPack Sealed (DK GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Manifold Absolute Pressure (MAP) Sensor Return
B | LT GRN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | GRY | 416 | Manifold Absolute Pressure (MAP) Sensor 5V Reference

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 12059595

• | 3-Way M Metri-Pack 150 Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | Mass Air Flow (MAF) Sensor Signal
B | BLK/WHT | 451 | Engine Control Module Ground
C | PNK | 639 | Ignition Feed

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY/BLK | 2701 | Throttle Position (TP) Sensor 5V Reference
B | BLK | 2752 | Throttle Position Sensor Return
C | DK BLU | 417 | Throttle Position Sensor Signal

#### Park/Neutral Position Switch C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 1737 | Transaxle Mounted Neutral Safety Switch Output
B | PNK | 539 | Fused Battery Feed
C | LT GRN | 275 | Transaxle Mounted Neutral Safety Switch Output
D | BLKWHT | 451 | Engine Control Module Ground
E | PPL | 6 | Starter Solenoid Feed
F | LT GRN | 24 | Backup Lamp Feed
G | YEL | 5 | Ignition Switch Output-Crank

#### Park Neutral Position Switch C2

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series Sealed (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | Signal Parity Bit
B | YEL | 772 | Switch Signal Bit 2
C | GRY | 773 | Switch Signal Bit 3
D | BLK/WHT | 771 | Switch Signal Bit 1

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | Vehicle Speed Sensor (VSS) Signal Return
B | YEL | 400 | Vehicle Speed Sensor (VSS) Signal