For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Back Up lamp Assembly to Rear Compartment Lid | 3 N·m | 53 lb in
Composite Headlamp Assembly Retaining Nuts | 8 N·m | 71 lb in
Fog Lamp to Impact Bar Retaining Nuts | 3 N·m | 53 lb in
High Mounted Stoplamp Socket to Lamp Assembly | 2 N·m | 17 lb in
License Lamp Retaining Nuts | 2 N·m | 17 lb in
Secondary Backup Light Retaining Nuts | 2 N·m | 17 lb in
Stoplamp to Rear Compartment Lid | 3 N·m | 53 lb in