For 1990-2009 cars

#### Coolant Level Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL/BLK | 68 | Low Coolant Level Indicator Control
B | BLK | 1350 | Ground

#### Cooling Fan-Left

Connector Part Information |

• | 12103172

• | 2-Way F Metri-Pack 630 Series Pull-to-Seat Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 504 | Cooling Fan Motor Ground
B | LT BLU | 409 | Cooling Fan Motor Supply Voltage

#### Cooling Fan-Right

Connector Part Information |

• | 12066681

• | 2-Way F Metri-Pack 630 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 450 | Ground
B | GRY | 532 | Cooling Fan Motor Supply Voltage