For 1990-2009 cars

Thermoset Plastic Type | Type of Repair | Recommended Repair Material | Availability
--- | --- | --- | ---
Most rigid plastic parts | Cosmetic filling | GM Goodwrench Structural Bonding Epoxy (GM P/N 12345726 or equivalent) | GM Dealer/Retailer
Sikkens Polystop LP or equivalent polyester repair putty | Refer to a local paint supplier
Most rigid plastic parts | Cosmetic repair; Adhesive bonding | GM Goodwrench Structural Bonding Epoxy (GM P/N 12345726 or equivalent) | GM Dealer/Retailer
Lord Fusor SMC Body Panel Repair Adhesive or equivalent | Refer to local paint supplier
Most rigid plastic parts | Adhesive bonding | GM Goodwrench Structural Bonding Epoxy (GM P/N 12345726 or equivalent) | GM Dealer/Retailer
Dynatron Dyna-Weld Plio Grip or equivalent (OE structural adhesive) | Refer to local paint supplier
Most rigid plastic parts | Adhesive structural* bonding | GM Goodwrench Structural Bonding Epoxy (GM P/N 12345726 or equivalent) | GM Dealer/Retailer
Most rigid plastic parts | Adhesive bonding Structural bonding | US Chemical and Plastic System 2000 Structural Adhesive P/N 82007B = 30 min P/N 82014B = 9 min | Refer to local paint supplier or US Chemicals customer service 1 800 321 0672
* Structural adhesive bonding may require the use of a pneumatic applicator, A8-37479-1A, or equivalent, to speed the application of the GM12345726 epoxy. | Kent-Moore 1-800-GM-TOOLS