For 1990-2009 cars

## Instrument Panel Outer Air Outlet Deflector Replacement - Left Side Oldsmobile

### Removal Procedure

1. With a suitable tool release the retaining tabs through the vanes of the HVAC air outlet deflector.
2. Pull the air deflector outlet out of the upper trim pad.

### Installation Procedure

1. Align the air deflector outlet to the opening in the upper trim pad.
2. Push the air deflector outlet into the upper trim pad until retaining tabs are engaged.