For 1990-2009 cars

The trim panel carpet is a one-piece molded unit.

### Removal Procedure

1. Remove the rear compartment sill trim plate. Refer to Rear Compartment Sill Trim Plate Replacement .
2. Remove the rear compartment spare tire storage cover. Refer to Spare Tire Cover Replacement .
3. Remove the cargo net. Refer to Cargo Net Replacement .
4. Remove the trim panel carpet retainers.
5. Remove the rear compartment trim (1).

### Installation Procedure

1. Install the rear compartment trim (1).
2. Install the trim panel carpet retainers.
3. Install the convenience net. Refer to Cargo Net Replacement .
4. Install the rear compartment spare wheel stowage cover. Refer to Spare Tire Cover Replacement .
5. Install the rear compartment sill trim plate. Refer to Rear Compartment Sill Trim Plate Replacement .