For 1990-2009 cars

Notice: When DTC B1018 or B1024 has been set it is necessary to replace the inflatable restraint Sensing and Diagnostic Module (SDM). Setting DTC B1018 or B1024 will also cause DTC B1071 to set. When a scan tool clear codes command is issued and the malfunction is no longer present, DTC B1018 or B1024 and DTC B1071 will remain current. Make sure that the short to ground condition is repaired prior to installing a replacement SDM to avoid damaging the SDM.