For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Wiper/Washer Schematics
1 | Did you review the Wiper/Washer System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Wiper/Washer Systems
2 | Turn the ignition ON. Are the windshield washers OFF? | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 | Disconnect the windshield wiper/washer switch connector. Do the windshield washers stop? | Go to Step 5 | Go to Step 4
4 | Test the windshield washer pump control circuit for a short to voltage. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 7 | Go to Step 6
5 | Replace the windshield wiper/washer switch. Is the repair complete? | Go to Step 7 | --
6 | Replace the windshield wiper motor module. Refer to Wiper Motor Cover Replacement . Is the repair complete? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3