For 1990-2009 cars

### Removal Procedure

1. Remove the rotor. Refer to Rear Brake Rotor Replacement in Disc Brakes.
2. Remove the parking brake actuator (2). Refer to Parking Brake Actuator Replacement .
3. Remove the rear wheel hub (8). Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
4. Remove the shoe and lining (7).

### Installation Procedure

1. Install shoe and lining (7).
2. Install the rear wheel hub. Refer to Rear Wheel Bearing and Hub Replacement in Rear Suspension.
3. Install the parking brake actuator (2). Refer to Parking Brake Actuator Replacement .
4. Adjust the rear parking brake shoe and lining. Refer to Parking Brake Shoe Adjustment .
5. Install the rotor. Refer to Rear Brake Rotor Replacement in Disc Brakes.