Engine Wiring. Chevrolet Beretta 1996

For 1990-2009 cars

Figure 1:

#### 2.2L

(1) | Coolant Temperature Lead
(2) | TCC Switch Connection
(3) | Negative Battery Cable
(4) | Engine Harness Ground Leads
(5) | Transmission Mounting Stud
(6) | Low Oil Level Lead
(7) | Positive Battery Cable
(8) | Oxygen Sensor
(9) | Coolant Fan Lead

Figure 2:

#### 2.2L

(1) | Oil Pressure Switch
(2) | VSS
(3) | Back-up Lamp Switch
(4) | Transmission Mount Bracket
(5) | Engine Wiring Harness

Figure 3:

#### 2.2L

(1) | Canister Purge
(2) | Oil Pressure Switch
(3) | VSS
(4) | Back-up Lamp Switch

Figure 4:

#### 2.2L

Figure 5:

#### Low Oil Level Sensor Wiring (2.2L)

(1) | Low Oil Level Sensor
(2) | Oil Pan
(3) | Starter Motor

Figure 6:

#### Starter Motor Wiring (2.2L)

(1) | Fusible Links
(2) | Positive Battery Cable
(3) | Low Oil Level Sensor Lead
(4) | Starter Motor

Figure 7:

#### TBI Wiring (2.2L)

(1) | IAC Motor Connection
(2) | Injector Harness Lead
(3) | EGR Solenoid Connection
(4) | MAT Sensor Connection
(5) | MAP Sensor Connection
(6) | TPS Sensor Connection

Figure 8:

#### A/C Compressor Wiring (2.2L)

(1) | Oxygen Sensor
(2) | A/C Transducer
(3) | Radiator Support
(4) | A/C Pipe
(5) | Generator

Figure 9:

#### 3100

(1) | IAC Sensor
(2) | EGR Solenoid
(3) | EGR Solenoid Lead
(4) | TPS Connector
(5) | MAT Sensor
(6) | ABS Wheel Sensor Lead
(7) | TCC Connector
(8) | Coolant Fan Lead

Figure 10:

#### 3100

(1) | Engine Wiring Harness Ground Leads
(2) | Engine Wiring Harness

Figure 11:

#### 3100

(1) | Ground Leads
(2) | Neutral Start Switch
(3) | Transmission Shift Cable Bracket
(4) | Engine Harness
(5) | Engine Harness Lead to Rear
(6) | MAT Sensor Lead
(7) | Front Left ABS Lead
(8) | TCC Connector

Figure 12:

#### Starter Harness Routing (L82)

(1) | Engine Wiring Harness
(2) | Oil Pressure Sensor
(3) | Starter Motor Assembly
(4) | Detonation Sensor
(5) | Oil Pan
(6) | A/C Compressor Clutch Connection
(7) | A/C Compressor
(8) | Water Pump
(9) | Crank Sensor Inter Connection

Figure 13:

#### 3100

(1) | Crankshaft Sensor
(2) | Low Oil Level Sensor Lead
(3) | Vehicle Speed Sensor

Figure 14:

#### 3100

(1) | Engine Wiring Harness
(2) | SIR Lead
(3) | Body Bracket
(4) | Radiator Overflow Bottle

Figure 15:

#### 3100

(1) | Right Coil Connection
(2) | Blower Motor Resistor Connector
(3) | Engine Wiring Harness
(4) | Oxygen Sensor
(5) | Left Coil Connection
(6) | TPS Lead
(7) | IAC Lead
(8) | EGR Solenoid Lead

Figure 16:

#### Master Cylinder Wiring

(1) | Brake Pressure Lead
(2) | ABS Solenoid Lead
(3) | 3-way ABS Motor Pack Lead
(4) | 6-way ABS Motor Pack Lead
(5) | Engine Harness

Figure 17:

#### Cooling Fan

(1) | A/C Line (L82 only)
(2) | Cooling Fan

Figure 18:

#### Bulkhead Connector

(1) | Forward Lamp Harness Bulkhead Connector
(2) | Hood Release Cable
(3) | Engine Harness
(4) | Fuel Pump Primer Lead
(5) | F.O.D. (Left Side)
(6) | Ground Lead

Figure 19:

#### ABS Motor Pack Wiring

(1) | Wiper Motor
(2) | Fluid Level Sensor
(3) | Air Cleaner Support
(4) | Engine Harness
(5) | EGR/IAC/TPS Branch (L82)