Engine Controls Components. Chevrolet Beretta 1996

For 1990-2009 cars

#### Engine Controls Component Location Table

Component | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
A/C Refrigerant Pressure Sensor And Fan Relay | RH Engine Compartment | 201-08, Fig 15 | -- | --
Automatic Transaxle | LH Front of Engine/Transaxle | 201-03, Fig 05 | 202-44 | --
Camshaft Position (CMP) Sensor | RH Rear of Engine | 201-05, Fig 9 | -- | --
Crankshaft Position (CKP) Sensor | Rear Center of Engine | 201-02, Fig 4 | -- | --
Data Link Connector (DLC) | LH Lower I/P | 201-19, Fig 37 | 202-11 | --
Linear Exhaust Gas Recirculation (EGR) Valve | L/H Front of Engine/Transaxle | 201-01, Fig 02 | 202-40 | --
Electronic Ignition Control Module (ICM) | Rear Center of Engine | 201-02, Fig 04 | -- | --
Engine Coolant Temperature (ECT) Sensor | LH Front of Engine/Transaxle | 201-03, Fig 05 | -- | --
Evaporative Emission Canister Purge Solenoid | Rear of Engine Below Intake Manifold | 201-02, Fig 04 | -- | --
Evaporative Emission Canister Purge Vacuum Switch | Rear Center of Engine | 201-02, Fig 04 | -- | --
Fuel Injectors | LH Top of Engine Compartment | 201-01, Fig 02 | -- | --
Fuel Pump Relay | Engine Compartment Front of Dash | 201-05, Fig 10 | 202-41 | --
Fuel Pump/Oil Pressure Sender/Switch | LH Rear of Engine | 201-02, Fig 04 | -- | --
Fuel Tank Unit | LH Rear Passenger Compartment | 201-14, Fig 27 | -- | --
Fuse Block | LH Lower I/P | 201-18, Fig 35 | -- | --
Fusible Link B | Lower Front of Engine | 201-09, Fig 17 | -- | --
Fusible Link E | Lower Front of Engine | 201-09, Fig 17 | -- | --
Idle Air Control (IAC) Valve | LH Top of Engine Compartment | 201-01, Fig 02 | 202-42 | --
Instrument Panel Cluster | LH Front of I/P | 201-19, Fig 38 | 202-18 | --
Intake Air Temperature (IAT) Sensor | Top of Engine | 201-01, Fig 02 | -- | --
Knock Sensor (KS) | Rear Center of Engine | 201-04, Fig 08 | -- | --
Manifold Absolute Pressure (MAP) Sensor | LH Top of Engine Compartment | 201-01, Fig 02 | -- | --
Oil Level Switch | LH Front of Engine/Transaxle | 201-03, Fig 05 | -- | --
Oxygen Sensor (O2S 1) | LH Front of Engine/Transaxle | 201-03, Fig 05 | -- | --
Park/Neutral Position (PNP) Switch | LH Rear of Engine Compartment On Transaxle | 201-02, Fig 04 | 202-43 | --
Powertrain Control Module (PCM) | RH Front of I/P | 201-06, Fig 12 | 202-24 | --
Rear Heated Oxygen Sensor (HO2S 2) | LH Rear of Engine Compartment | 201-06, Fig 11 | 202-44 | --
Throttle Position (TP) Sensor | LH Top of Engine Compartment | 201-01, Fig 02 | -- | --