Thermo Element Replacement. Chevrolet Beretta 1996

For 1990-2009 cars

### Removal Procedure

1. Remove the transmission mount. Refer to Transmission Mount Replacement .
2. Remove the transmission mount bracket.
3. Remove the valve body cover. Refer to Valve Body Cover Replacement .
4. Remove the case cover. Refer to Case Cover Replacement .
5. Inspect the thermo element washers.
6. Inspect the thermo element.
7. Inspect the thermo element plate.

### Installation Procedure

1. Install the case cover. Refer to Case Cover Replacement .
2. Install the valve body cover. Refer to Valve Body Cover Replacement .
3. Install the transmission mount bracket.
4. Install the transmission mount. Refer to Transmission Mount Replacement .