For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Axle Shaft Mounting Nut

- 12 stud axle

77 N·m

57 lb ft

- 8 stud axle

155 N·m

114 lb ft

Axle Vent Assembly | 14 N·m | 124 lb in
Differential Carrier to Axle Housing Bolt-Eaton®

- Models 15040S and 19050S

128 N·m

94 lb ft

- Model 19050T

143 N·m

105 lb ft

- Model DS404

222 N·m

164 lb ft

- Models 19060S, 19060T, 21060S, 21060T, 22060S, 22060T, 23080S, 23080T, and 23105S

227 N·m

167 lb ft

Differential Carrier to Axle Housing Bolt-Dana/Spicer® Model S150-S | 150 N·m | 111 lb ft
Drain Plug | 70 N·m | 52 lb ft
Drive Pinion Nut-Dana/Spicer® Model S150-S | 1088 N·m | 802 lb ft
Drive Pinion Nut-Eaton®

- Models 15040S, 19050S, and 19050T

568 N·m

419 lb ft

- Models 15060S, 21060S, and 22060S

867 N·m

639 lb ft

- Models 15060T, 21060T, and 22060T

1025 N·m

755 lb ft

Drive Pinion Nut-Eaton®

- Model 23080T

1190 N·m

877 lb ft

- Models 23080S and 23105S

1262 N·m

930 lb ft

- Rear Unit Model DS404

867 N·m

639 lb ft

Output Shaft Nut-Eaton® Model DS404 | 1025 N·m | 755 lb ft
Rear Axle Fill Plug | 33 N·m | 24 lb ft
Rear Wheel Bearing Outer Nut | 169 N·m | 125 lb ft
Spindle Key-Way Nut | 103.5 N·m | 77 lb ft
Top-Off Plug | 67 N·m | 49 lb ft
Two Speed Rear Axle Pressure Protection Valve Nuts | 12 N·m | 106 lb in
Two Speed Rear Axle Shift Motor Nuts | 74 N·m | 55 lb ft
Two Speed Rear Axle Shift Quick Release Valve Nuts | 22 N·m | 16 lb ft
Wire Harness Clip Nuts | 1.9 N·m | 17 lb in