For 1990-2009 cars

Problem | Action
--- | ---
DEFINITION: A noise is present when the vehicle turns.
The differential side gears and the pinion gears are worn. | Replace the worn parts. Spicer Eaton call 1-800-TCM-HELP Meritor 1-800-535-5560
The differential spider is worn. | Replace the worn parts. Spicer Eaton call 1-800-TCM-HELP Meritor 1-800-535-5560
The rear axle shaft splines are worn. | Replace the rear axle shafts. Refer to Rear Axle Shaft and/or Gasket Replacement .