For 1990-2009 cars

### Removal Procedure

1. Disconnect the clutch engine brake switch electrical harness connector.
2. Remove the clutch engine brake switch retainer.
3. Remove the clutch engine brake switch.

### Installation Procedure

1. Install the clutch engine brake switch.
2. Install the clutch engine brake switch retainer.
3. Connect the clutch engine brake switch electrical harness connector.