For 1990-2009 cars

Figure 1: |

#### Engine Harness to Engine (LG5), Right Side

(1) | Engine Coolant Temperature (ECT) Switch (UER)
(2) | Generator

Figure 2: |

#### Engine Harness to Starter, Right Side Front View

(1) | Engine Harness
(2) | C106a/C106b
(3) | Starter Temperature Switch, HD Starter with Overcrank Protection
(4) | Starter

Figure 3: |

#### Positive Battery Cable to Engine Components, Right Front View

(1) | Starter Solenoid
(2) | Starter
(3) | Engine Harness
(4) | G101
(5) | G103
(6) | Positive Battery Cable
(7) | G124

Figure 4: |

#### Relays-Lower Exterior Bulkhead, Right Side

(1) | Automatic Transmission Modulator Relay
(2) | Starter Relay
(3) | Engine Brake Relay (LG5/K40)
(4) | Bulkhead