For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Air Brake Chamber Clevis Jam Nut (Type 16 Service Air Brake Chamber) | 45 N·m | 33 lb ft
Front Air Brake Chamber Clevis Jam Nut (Types 20 and 24 Service Air Brake Chamber) | 78 N·m | 57 lb ft
Front Cam Brake Assembly Bolt | 280 N·m | 206 lb ft
Rear Air Brake Chamber Clevis Jam Nut | 77 N·m | 56 lb ft
Rear Cam Brake Assembly Bolt | 220 N·m | 162 lb ft
Release Stud Nut (Maximum Torque for Caging the Spring Brake Chamber Assembly) | 47 N·m | 35 lb ft
Release Stud Nut (Tool Storage) | 7 N·m | 62 lb in
Service Brake Automatic Slack Adjuster Control Arm Nut | 17 N·m | 13 lb ft
Service Brake Chamber Assembly Mounting Nut (Type 16) | 39 N·m | 29 lb ft
Service Brake Chamber Assembly Mounting Nut (Types 20 and 24) | 74 N·m | 55 lb ft
Service Brake Chamber Clamp Ring Assembly Nut | 34 N·m | 25 lb ft
Spring Brake Chamber Assembly Mounting Nut | 108 N·m | 80 lb ft
Spring Brake Chamber Clamp Ring Assembly Nut | 34 N·m | 25 lb ft