For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cushion Bracket Nuts | 45 N·m | 33 lb ft
Cushion Support Nuts | 31 N·m | 23 lb ft
Modulator Clip Bolt | 20 N·m | 15 lb ft
Oil Cooler Line Nuts to Oil Filter Adapter | 30 N·m | 22 lb ft
Oil Cooler Line Nuts to Transmission and Radiator Connectors | 25 N·m | 18 lb ft
Oil Level Indicator Tube Bolts and Nuts | 20 N·m | 15 lb ft
Support Beam Nuts | 105 N·m | 77 lb ft
Torque Converter to Flywheel Bolts (7.2L and 2000/2400) | 60 N·m | 44 lb ft
Torque Converter to Flywheel Bolts (7.2L and AT545) | 67 N·m | 49 lb ft
Torque Converter to Flywheel Bolts (7.2L and MT643/MT653) | 67 N·m | 49 lb ft
Torque Converter to Flywheel Bolts (7.2L and MD3060P/MD3560P) | 40 N·m | 30 lb ft
Torque Converter to Flywheel Bolts (7.2L and MD3080P/MD3580P) | 45 N·m | 33 lb ft
Torque Converter to Flywheel Bolts (8.1L and 2000/2400) | 60 N·m | 44 lb ft
Torque Converter to Flywheel Bolts (8.1L and AT545) | 55 N·m | 41 lb ft
Torque Converter to Flywheel Bolts (8.1L and MT643/MT653) | 50 N·m | 37 lb ft
Transmission to Engine Bolts | 55 N·m | 41 lb ft
Vacuum Line Bolts and Nuts | 23 N·m | 17 lb ft

Application | Specifications
--- | ---
Metric | English
Control Valve Body Assembly to Transmission Case | 12 N·m | 108 lb in
Manual Shift Shaft Detent Spring to Control Valve Body Assembly | 12 N·m | 108 lb in
Flange/Yoke to Output Shaft | 123 N·m | 91 lb ft
Transmission Oil Pump Cover Assembly to Torque Converter Housing | 56 N·m | 42 lb ft
Input Speed Sensor to Torque Converter Housing | 12 N·m | 108 lb in
Oil Pump Assembly to Transmission Oil Pump Cover Assembly | 26 N·m | 20 lb ft
Park/Neutral Position Switch to Transmission Case | 28 N·m | 22 lb ft
Oil Pan to Transmission Case | 26 N·m | 20 lb ft
Output Speed Sensor to Low and Reverse Clutch Piston Housing | 12 N·m | 108 lb in
Transmission Fluid Pressure Switch to Main Valve Body Assembly | 12 N·m | 108 lb in
Power Take-Off (PTO) Cover to Transmission Case | 43 N·m | 32 lb ft
Low and Reverse Clutch Piston Housing to Transmission Case | 56 N·m | 42 lb ft
Manual Shift Shaft Nut | 24 N·m | 17 lb ft
Shift Valve Body to Main Valve Body | 12 N·m | 108 lb in
Shipping Bracket to Torque Converter Assembly | 27 N·m | 20 lb ft
Turbine Speed Sensor to Transmission Case | 12 N·m | 108 lb in