For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Auxillary Air Compressor Nuts | 70 N·m | 52 lb ft
Auxillary Air Compressor Tank | 25 N·m | 18 lb ft
Catalytic Converter Hanger Clamp Nut | 29 N·m | 21 lb ft
Catalytic Converter to Muffler Flange Nuts | 64 N·m | 47 lb ft
Exhaust Hanger Nut | 24 N·m | 18 lb ft
Exhaust Manifold Bolt L18 | 35 N·m | 26 lb ft
Exhaust Manifold Nut 7.8L | 34 N·m | 25 lb ft
Exhaust Manifold Nuts 6.6L | 34 N·m | 25 lb ft
Exhaust Pipe to Exhaust Manifold 6.6L | 53 N·m | 39 lb ft
Exhaust Manifold Heat Shield 6.6L | 8 N·m | 71 lb in
Exhaust Manifold Nut L18 | 16 N·m | 12 lb ft
Exhaust Manifold Heat Shield NutL18 | 25 N·m | 18 lb ft
Exhaust Manifold Pipe Nuts (L18) | 50 N·m | 39 lb ft
Exhaust Pipe Bracket Clamp Nut | 24 N·m | 18 lb ft
Exhaust Pipe Hanger Bracket Bolt | 12 N·m | 106 lb in
Exhaust Pipe Clamp 6.6L | 40 N·m | 30 lb ft
Exhaust Muffler Nuts 6.6L | 40 N·m | 30 lb ft
Flexpipe Band Clamp | 24 N·m | 18 lb ft
Muffler Clamp Nut (L18) | 60 N·m | 44 lb ft
Muffler Clamp Nut (LG5) | 73 N·m | 54 lb ft
Tailpipe Bracket Nut | 10 N·m | 89 lb in
Tailpipe Cap Nut | 5 N·m | 44 lb in
Tailpipe Clamp Nut | 29 N·m | 21 lb ft
Transmission Bolt | 100 N·m | 74 lb ft
Turbocharger/Exhaust Brake Clamp | 10 N·m | 89 lb in
Upper Tailpipe Heat Shield Nut | 25 N·m | 18 lb ft
Wide Band Clamp | 73 N·m | 54 lb ft