For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 48 N·m | 35 lb ft
Clutch Cable Bracket Bolt - to Transmission | 93 N·m | 69 lb ft
Clutch Cable Bracket Bolt - to Transmission | 36 N·m | 27 lb ft
Clutch Cable Bracket Nut | 36 N·m | 27 lb ft
Clutch Cable Bracket Nut - to Support | 23 N·m | 17 lb ft
Control Lever Boot Bolt | 2 N·m | 18 lb in
Control Lever Boot Retainer Plate Bolt | 2 N·m | 18 lb in
Control Lever Retainer Bolt | 2 N·m | 18 lb in
Control Lever Set Screw | 39 N·m | 28 lb ft
Control Lever Sheath Screw | 5 N·m | 44 lb in
Exhaust Manifold Front Pipe Clamp Nut | 10 N·m | 89 lb in
Exhaust Manifold Front Pipe U-Bolt Nut | 24 N·m | 18 lb ft
Flywheel Housing Bolt | 67 N·m | 49 lb ft
Flywheel Housing Cover Bolt | 12 N·m | 106 lb in
Housing Cover Extension Bolt | 43 N·m | 32 lb ft
Oil Drain and Fill Plugs - Spicer® | 45 N·m | 33 lb ft
Oil Drain Plug - Eaton Fuller® | 61 N·m | 45 lb ft
Oil Fill Plug - Eaton Fuller® | 82 N·m | 60 lb ft
Propeller Shaft Yoke Nut | 441 N·m | 325 lb ft
Rear Bearing Cover Bolt/Nut | 33 N·m | 24 lb ft
Shift Knob Lock Nut | 25 N·m | 18 lb ft
Transmission Bolt | 50 N·m | 37 lb ft
Transmission Boot Bolt | 2 N·m | 18 lb in
Transmission Boot Retainer Bolt | 2 N·m | 18 lb in
Transmission Mount Bracket Nut | 71 N·m | 52 lb ft
Transmission Mount Nut | 46 N·m | 34 lb ft
Transmission Nut | 163 N·m | 120 lb ft
Transmission Support Bolt | 195 N·m | 144 lb ft
Transmission Support Nut | 31 N·m | 23 lb ft
Vehicle Speed Sensor | 48 N·m | 35 lb ft