For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Directional and Parking Lamp Backing Plate Retaining Nut | 8 N·m | 71 lb in
Headlamp Bezel Screw | 1.9 N·m | 17 lb in
Parking Brake Switch, C Model with Air Brakes, Switch | 12 N·m | 106 lb in
Parking Brake Switch, C Model with Hydraulic Brakes, Retaining Screw | 4.5 N·m | 40 lb in
Tail Lamp Assembly Retaining Bolt | 35 N·m | 26 lb ft