For 1990-2009 cars

## Fuel Filter Replacement Primary

### Removal Procedure

1. Relieve the fuel system pressure.
2. Remove the fuel filter from the fuel filter head.

Important: If the fuel filter is plugged, inspect the fuel tank internally and clean if necessary. Refer to Fuel System Cleaning .

3. Inspect the fuel filter.

### Installation Procedure

1. Install the fuel filter.
2. Inspect for leaks.