For 1990-2009 cars

### Removal Procedure

1. Remove the wiper blade from the wiper arm. Refer to Windshield Wiper Blade Replacement .

Important: The wiper blade element must be replaced if removed.

2. Remove the wiper blade element from the wiper blade by squeezing the locking tabs together, and pull the element from the wiper blade.

### Installation Procedure

1. Install the wiper blade element into the wiper blade.

1.1. | Position the wiper blade element at the bottom end of the wiper blade.

1.2. | Guide the wiper blade element through the wiper blade, making sure to engage the claw sets along the entire length of the blade.

1.3. | The element is fully seated when both of the locking tabs engage the claw set.

2. Install the wiper blade onto the wiper arm. Refer to Windshield Wiper Blade Replacement .