For 1990-2009 cars

### Removal Procedure

1. Apply the parking brake.
2. Remove the MaxiFuse® block (1) cover.

Pull down and remove the parking brake pump relay (3) from the bracket.

3. Remove the parking brake pump relay electrical connector (2).

### Installation Procedure

1. Install the parking brake pump relay electrical connector (2).
2. Install the parking brake pump relay (3) to the bracket.
3. Install the MaxiFuse® block (1) cover.