For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Combination Valve to BPMV | 16 N·m | 12 lb ft
EBCM Bracket Mounting Bolts | 36 N·m | 28 lb ft
EBCM to BPMV | 5 N·m | 44 lb in
EHCU to Bracket | 9 N·m | 7 lb ft
EHCU Crossmember Bolts | 36 N·m | 28 lb ft
Front Brake Line to Combination Valve | 24 N·m | 18 lb ft
Front Wheel Speed Sensor Mounting Bolts | 26 N·m | 19 lb ft
Hydraulic Lines to Tube Adapters | 30 N·m | 22 lb ft
Rear Brake Line to Combination Valve | 24 N·m | 18 lb ft
Splash Shield Mounting Bolts | 11 N·m | 9 lb ft
Tube Adapters to BPMV | 31 N·m | 23 lb ft
Wheel Speed Sensor Harness Clip to Shock Tower | 11 N·m | 9 lb ft