For 1990-2009 cars

### Removal Procedure

1. Pull down the dome lamp lens in order to remove the bulb.
2. Remove the dome lamp bulb as follows:

2.1. | Grasp the bulb in the center.

2.2. | Push the bulb toward one of the spring clips in order to free the other end of the bulb.

### Installation Procedure

1. Install the dome lamp bulb by pushing the bulb straight into the housing until it is fully seated.
2. Push up the dome lamp lens in order to install.