For 1990-2009 cars

Table 1: | C101
Table 2: | C102
Table 3: | C104
Table 4: | C105
Table 5: | C106a/C106b
Table 6: | C107
Table 7: | C109
Table 8: | C110
Table 9: | C112
Table 10: | C113
Table 11: | C115
Table 12: | C119
Table 13: | C123
Table 14: | C124
Table 15: | C125
Table 16: | C127
Table 17: | C200
Table 18: | C201
Table 19: | C202
Table 20: | C204 (with A/C)
Table 21: | C204 (without A/C)
Table 22: | C205
Table 23: | C206
Table 24: | C207
Table 25: | C208
Table 26: | C210
Table 27: | C215
Table 28: | C218
Table 29: | C219
Table 30: | C220
Table 31: | C221
Table 32: | C222
Table 33: | C223
Table 34: | C225
Table 35: | C226
Table 36: | C227
Table 37: | C228
Table 38: | C229
Table 39: | C230
Table 40: | C403
Table 41: | C404
Table 42: | C405
Table 43: | C406
Table 44: | C408
Table 45: | C409
Table 46: | C411
Table 47: | C412
Table 48: | C419

#### C101

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 150 | Ground (L18) | A | BLK | 150 | Ground (L18)
A | BLK | 650 | Ground (LG5) | A | BLK | 650 | Ground (LG5)
B | DK GRN | 29 | Horn Control | B | DK GRN | 29 | Horn Control

#### C102

Connector Part Information |

• | 12059472

• | 7 Way F Metri-Pack Mixed Series, Sealed (BLK)

Connector Part Information

• | 12052200

• | 7 Way M Metri-Pack Mixed Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Supply Voltage | A | BRN | 9 | Park Lamp Supply Voltage
B | TAN | 12 | Headlamp Low Beam Supply Voltage | B | TAN | 12 | Headlamp Low Beam Supply Voltage
C | LT BLU | 14 | Left Turn Signal Lamps Supply Voltage | C | LT BLU | 14 | Left Turn Signal Lamps Supply Voltage
D | DK BLU | 15 | Right Turn Signal Lamps Supply Voltage | D | DK BLU | 15 | Right Turn Signal Lamps Supply Voltage
E | LT GRN | 11 | Headlamp High Beam Supply Voltage | E | LT GRN | 11 | Headlamp High Beam Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used
G | BLK | 150 | Ground | G | BLK | 150 | Ground

#### C104

Connector Part Information |

• | 12124685

• | 3 Way F Metri-Pack 630 Series, Sealed (BLK)

Connector Part Information

• | 12124686

• | 3 Way M Metri-Pack 630 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1930 | Park Brake Motor Supply Voltage | A | ORN | 1930 | Park Brake Motor Supply Voltage
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | -- | -- | Not Used | C | -- | -- | Not Used

#### C105

Connector Part Information |

• | 12047937

• | 8 Way F Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12047931

• | 8 Way M Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL/BLK | 1931 | Park Brake Pressure Valve Solenoid Supply Voltage | A | YEL/BLK | 1931 | Park Brake Pressure Valve Solenoid Supply Voltage
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | TAN | 1935 | Service Park Brake Indicator Supply Voltage | C | TAN | 1935 | Service Park Brake Indicator Supply Voltage
D | BLK | 250 | Ground | D | BLK | 250 | Ground
E | LT GRN/BLK | 1087 | Park Brake Pressure Sensor Low Reference | E | LT GRN/BLK | 1087 | Park Brake Pressure Sensor Low Reference
F | PNK | 1086 | Park Brake Pressure Sensor Voltage Reference | F | PNK | 1086 | Park Brake Pressure Sensor Voltage Reference
G | LT GRN | 1088 | Park Brake Pressure Sensor Signal | G | LT GRN | 1088 | Park Brake Pressure Sensor Signal
H | -- | -- | Not Used | H | -- | -- | Not Used

#### C106a/C106b

Connector Part Information |

• | 12065172

• | 1 Way F Metri-Pack 280 Series, Sealed (BLK)

Connector Part Information

• | 12065171

• | 1 Way M Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 434 | Neutral Safety Switch Signal | A | ORN/BLK | 434 | Neutral Safety Switch Signal

#### C107

Connector Part Information |

• | 12129613

• | 7 Way F Metri-Pack 280 Series, Sealed (GRY)

Connector Part Information

• | 12129614

• | 7 Way M Metri-Pack 280 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 471 | Trailer ABS Indicator Control- Late Production | A | WHT | 471 | Trailer ABS Indicator Control-Late Production
B | BRN | 1941 | Ignition 3 Voltage | B | BRN | 1941 | Ignition 3 Voltage
C | PNK | 1905 | Retarder Disable Control | C | PNK | 1905 | Retarder Disable Control
D | WHT/BLK | 1922 | SAE J1708 Serial Data B | D | WHT/BLK | 1922 | SAE J1708 Serial Data B
E | TAN/BLK | 1921 | SAE J1708 Serial Data A | E | TAN/BLK | 1921 | SAE J1708 Serial Data A
F | DK BLU | 1899 | Brake Lamp Relay Control | F | DK BLU | 1899 | Brake Lamp Relay Control
G | -- | -- | Not Used | G | -- | -- | Not Used

#### C109

Connector Part Information |

• | 12047938

• | 8 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12047933

• | 8 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 650 | Ground | A | BLK | 650 | Ground
B | RED | 2127 | IC 7 Control | B | RED | 2127 | IC 7 Control
C | DK GRN | 2125 | IC 5 Control | C | DK GRN | 2125 | IC 5 Control
E | BRN | 2129 | Low Reference | E | BRN | 2129 | Low Reference
F | LT BLU | 2123 | IC 3 Control | F | LT BLU | 2123 | IC 3 Control
G | PPL | 2121 | IC 1 Control | G | PPL | 2121 | IC 1 Control
H | PNK | 139 | Ignition 1 Voltage | H | PNK | 139 | Ignition 1 Voltage

#### C110

Connector Part Information |

• | 12047938

• | 8 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12047933

• | 8 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 650 | Ground | A | BLK | 650 | Ground
B | RED/ WHT | 2122 | IC 2 Control | B | RED | 2122 | IC 2 Control
C | DK GRN/ WHT | 2124 | IC 4 Control | C | DK GRN | 2124 | IC 4 Control
E | BRN/ WHT | 2130 | Low Reference | E | BRN | 2130 | Low Reference
F | LT BLU/ WHT | 2126 | IC 6 Control | F | LT BLU | 2126 | IC 6 Control
G | PPL/ WHT | 2128 | IC 8 Control | G | PPL | 2128 | IC 8 Control
H | PNK | 239 | Ignition 1 Voltage | H | PNK | 239 | Ignition 1 Voltage

#### C112

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK/WHT | 1962 | Engine Brake Solenoid Feed | A | BLK/WHT | 1962 | Engine Brake Solenoid Feed
B | BLK | 650 | Ground | B | BLK | 650 | Ground

#### C113

Connector Part Information |

• | 12052641

• | 2 Way F Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12052647

• | 2 Way M Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 1507 | Service Trans Filter Indicator Control | A | RED | 1507 | Service Trans Filter Indicator Control
B | BLK | 150 | Ground | B | BLK | 150 | Ground

#### C115

Connector Part Information |

• | 12052641

• | 2 Way F Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12052647

• | 2 Way M Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage | A | PNK | 39 | Ignition 1 Voltage
B | LT BLU | 1998 | Intake Air Heater Indicator Control | B | LT BLU | 1998 | Intake Air Heater Indicator Control

#### C119

Connector Part Information |

• | 12059472

• | 7 Way F Metri-Pack Mixed, Sealed (BLK)

Connector Part Information

• | 112052200

• | 7 Way M Metri-Pack Mixed, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TAN | 848 | Brake Switch Signal | A | TAN | 848 | Brake Switch Signal
B | LT GRN | 867 | ABS Indicator Failure Control | B | LT GRN | 867 | ABS Indicator Failure Control
C | DK BLU | 1899 | Brake Lamp Relay Control | C | DK BLU | 1899 | Brake Lamp Relay Control
D | PPL | 333 | Brake Fluid Level Sensor Signal-Early LG5 Only | D | PPL | 333 | Brake Fluid Level Sensor Signal-Early LG5 Only
D | PNK | 1905 | Retarder Disable Control-Late LG5 Only | D | PNK | 1905 | Retarder Disable Control-Late LG5 Only
E | BRN | 341 | Ignition 3 Voltage | E | BRN | 341 | Ignition 3 Voltage
F | TAN/WHT | 799 | ABS Serial Data | F | TAN/WHT | 799 | ABS Serial Data
G | RED | 142 | Battery Positive Voltage | G | RED | 142 | Battery Positive Voltage

#### C123

Connector Part Information |

• | 12124685

• | 3 Way F Metri-Pack 630 Series (BLK)

Connector Part Information

• | 12124686

• | 3 Way M Metri-Pack 630 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 2 | Battery Positive Voltage | A | RED | 2 | Battery Positive Voltage
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | RED | 442 | Battery Positive Voltage | C | RED | 442 | Battery Positive Voltage

#### C124

Connector Part Information |

• | 15300027

• | 2 Way F Metri-Pack 280 Series, Sealed (BLK)

Connector Part Information

• | 15300002

• | 2 Way M Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN/BLK | 434 | Neutral Safety Switch Signal | A | ORN/BLK | 434 | Neutral Safety Switch Signal
B | BLK | 150 | Ground | B | BLK | 150 | Ground

#### C125

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage | A | BRN | 241 | Ignition 3 Voltage
B | BLK | 650 | Ground | B | BLK | 650 | Ground

#### C127

Connector Part Information |

• | 12065425

• | 10 Way F Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12048253

• | 10 Way M Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 1744 | Fuel Injector 1 Control | A | BLK | 1744 | Fuel Injector 1 Control
B | DK BLU/ WHT | 878 | Fuel Injector 8 Control | B | DK BLU/ WHT | 878 | Fuel Injector 8 Control
C | LT BLU/ BLK | 844 | Fuel Injector 4 Control | C | LT BLU/ BLK | 844 | Fuel Injector 4 Control
D | PNK/ BLK | 1746 | Fuel Injector 3 Control | D | PNK/ BLK | 1746 | Fuel Injector 3 Control
E | YEL/ BLK | 846 | Fuel Injector 6 Control | E | YEL/ BLK | 846 | Fuel Injector 6 Control
F | BLK/ WHT | 845 | Fuel Injector 5 Control | F | BLK/ WHT | 845 | Fuel Injector 5 Control
G | RED/ BLK | 877 | Fuel Injector 7 Control | G | RED/ BLK | 877 | Fuel Injector 7 Control
H | LT GRN/ BLK | 1745 | Fuel Injector 2 Control | H | LT GRN/ BLK | 1745 | Fuel Injector 2 Control
J | PNK | 139 | Ignition 1 Voltage | J | PNK | 139 | Ignition 1 Voltage
K | PNK | 239 | Ignition 1 Voltage | K | PNK | 239 | Ignition 1 Voltage

#### C200

Connector Part Information |

• | 12034257

• | 56 Way F Metri-Pack Mixed Series (BLK)

Connector Part Information

• | 12066434

• | 56 Way M Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | DK GRN | 1049 | Class 2 Serial Data (MTW/MX4) | A1 | DK GRN | 1049 | Class 2 Serial Data (MTW/MX4)
A1 | -- | -- | Not Used-All Others | A1 | -- | -- | Not Used-All Others
A2 | BRN | 241 | Ignition 3 Voltage | A2 | BRN | 241 | Ignition 3 Voltage
A3 | LT BLU | 14 | Left Turn Signal Lamp Supply Voltage | A3 | LT BLU | 14 | Left Turn Signal Lamp Supply Voltage
A4 | BRN | 541 | Ignition 3 Voltage (L18) | A4 | BRN | 541 | Ignition 3 Voltage (L18)
A4 | GRY | 397 | Cruise Control On Switch Signal (LG5) | A4 | GRY | 397 | Cruise Control On Switch Signal (LG5)
A6 | BLK | 250 | Ground | A6 | BLK | 250 | Ground
A7 | DK GRN | 29 | Horn Control | A7 | DK GRN | 29 | Horn Control
A8 | DK GRN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | A8 | DK GRN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
A9 | YEL | 18 | Left Rear Stop/Turn Lamp Supply Voltage | A9 | YEL | 18 | Left Rear Stop/Turn Lamp Supply Voltage
B1 | PNK | 139 | Ignition 1 Voltage (L18) | B1 | PNK | 139 | Ignition 1 Voltage (L18)
B1 | WHT/BLK | 448 | Powertrain Diagnostic Enable (LG5) | B1 | WHT/BLK | 448 | Powertrain Diagnostic Enable (LG5)
B2 | -- | -- | Not Used (L18) | B2 | -- | -- | Not Used (L18)
B2 | ORN | 2240 | Battery Positive Voltage (LG5) | B2 | ORN | 2240 | Battery Positive Voltage (LG5)
B3 | DK BLU | 15 | Right Turn Signal Lamps Supply Voltage | B3 | DK BLU | 15 | Right Turn Signal Lamps Supply Voltage
B4 | -- | -- | Not Used (L18) | B4 | -- | -- | Not Used (L18)
B4 | TAN/BLK | 231 | Oil Pressure Switch Signal (LG5) | B4 | TAN/BLK | 231 | Oil Pressure Switch Signal (LG5)
B6 | PNK | 239 | Ignition 1 Voltage (L18) | B6 | PNK | 239 | Ignition 1 Voltage (L18)
B6 | WHT/BLK | 1922 | SAE J1708 Serial Data B (LG5) | B6 | WHT/BLK | 1922 | SAE J1708 Serial Data B (LG5)
B7 | -- | -- | Not Used (L18) | B7 | -- | -- | Not Used (L18)
B7 | TAN/BLK | 1921 | SAE J1708 Serial Data A (LG5) | B7 | TAN/BLK | 1921 | SAE J1708 Serial Data A (LG5)
B8 | LT GRN | 448 | PTO On Switch Signal (L18) | B8 | LT GRN | 448 | PTO On Switch Signal (L18)
B8 | PNK | 439 | Ignition 1 Voltage (MTW/MX4) | B8 | PNK | 439 | Ignition 1 Voltage (MTW/MX4)
B8 | -- | -- | Not Used - All Others | B8 | -- | -- | Not Used - All Others
B9 | WHT | 22 | Ground (RQ3/U86) | B9 | WHT | 22 | Ground (RQ3/U86)
C1 | -- | -- | Not Used (L18) | C1 | -- | -- | Not Used (L18)
C1 | BRN/WHT | 419 | MIL Control (LG5) | C1 | BRN/WHT | 419 | MIL Control (LG5)
C2 | PPL | 30 | Fuel Level Sensor Signal | C2 | PPL | 30 | Fuel Level Sensor Signal
C3 | DK GRN | 135 | Coolant Temperature Sensor Signal | C3 | DK GRN | 135 | Coolant Temperature Sensor Signal
C4 | -- | -- | Not Used (L18) | C4 | -- | -- | Not Used (L18)
C4 | WHT | 1961 | Engine Brake Switch Output (K40) | C4 | WHT | 1961 | Engine Brake Switch Output (K40)
C6 | -- | -- | Not Used (L18) | C6 | -- | -- | Not Used (L18)
C6 | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal (LG5) | C6 | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal (LG5)
C7 | DK GRN | 534 | High Idle Switch Output | C7 | DK GRN | 534 | High Idle Switch Output
C8 | GRY | 1148 | Transmission Shift Inhibit Signal (MTW/MX4) | C8 | GRY | 1148 | Transmission Shift Inhibit Signal (MTW/MX4)
C8 | -- | -- | Not Used-All Others | C8 | -- | -- | Not Used-All Others
C9 | LT GRN | 1478 | Coolant Level Switch Signal | C9 | LT GRN | 1478 | Coolant Level Switch Signal
D1 | -- | -- | Not Used (L18) | D1 | -- | -- | Not Used (L18)
D1 | LT GRN/ BLK | 822 | Vehicle Speed Sensor Low Signal-Early LG5 | D1 | LT GRN/ BLK | 822 | Vehicle Speed Sensor Low Signal-Early LG5
D1 | ORN | 40 | Battery Positive Voltage (MWF/MTW/MX4) | D1 | ORN | 40 | Battery Positive Voltage (MWF/MTW/MX4)
D2 | YEL | 53 | Generator Fuse Output | D2 | YEL | 53 | Generator Fuse Output
D3 | -- | -- | Not Used (L18) | D3 | -- | -- | Not Used (L18)
D3 | ORN/BLK | 434 | Neutral Safety Switch Signal (LG5) | D3 | ORN/BLK | 434 | Neutral Safety Switch Signal (LG5)
D6 | PPL | 420 | TCC Brake Switch Signal (L18) | D6 | PPL | 420 | TCC Brake Switch Signal (L18)
D6 | DK BLU | 84 | Cruise Control Set/Coast Switch Signal (LG5) | D6 | DK BLU | 84 | Cruise Control Set/Coast Switch Signal (LG5)
D7 | -- | -- | Not Used (L18) | D7 | -- | -- | Not Used (L18)
D7 | BLK | 808 | Low Reference (LG5) | D7 | BLK | 808 | Low Reference (LG5)
D8 | -- | -- | Not Used (L18) | D8 | -- | -- | Not Used (L18)
D8 | DK BLU | 417 | TP Sensor Signal (LG5) | D8 | DK BLU | 417 | TP Sensor Signal (LG5)
E1 | -- | -- | Not Used-L18/Late LG5 | E1 | -- | -- | Not Used-L18/Late LG5
E1 | PPL/WHT | 821 | VSS High Signal-Early LG5 | E1 | PPL/WHT | 821 | VSS High Signal-Early LG5
E2 | -- | -- | Not Used (L18) | E2 | -- | -- | Not Used (L18)
E2 | TAN/WHT | 331 | Oil Pressure Sensor Signal (LG5) | E2 | TAN/WHT | 331 | Oil Pressure Sensor Signal (LG5)
E3 | -- | -- | Not Used | E3 | -- | -- | Not Used
E4 | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal (L18) | E4 | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal (L18)
E4 | YEL | 1389 | Vehicle Speed Signal-Early LG5 | E4 | YEL | 1389 | Vehicle Speed Signal-Early LG5
E4 | DK GRN | 389 | Vehicle Speed Signal-Late LG5 | E4 | DK GRN | 389 | Vehicle Speed Signal-Late LG5
E6 | -- | -- | Not Used (L18) | E6 | -- | -- | Not Used (L18)
E6 | BRN | 1675 | Check Gages Indicator Control (LG5) | E6 | BRN | 1675 | Check Gages Indicator Control (LG5)
E7 | RED | 2013 | High Idle Indicator Control | E7 | RED | 2013 | High Idle Indicator Control
E8 | -- | -- | Not Used (L18) | E8 | -- | -- | Not Used (L18)
E8 | LT GRN/ BLK | 431 | 8 Volt Reference (LG5) | E8 | LT GRN/ BLK | 431 | 8 Volt Reference (LG5)
E9 | -- | -- | Not Used | E9 | -- | -- | Not Used
E9 | GRY | 1234 | Do Not Shift Indicator Control-Early MWF | E9 | GRY | 1234 | Do Not Shift Indicator Control -Early MWF
E9 | BRN/WHT | 1034 | Check Trans Indicator Control-Late MWF/MTW/MX4 | E9 | BRN/WHT | 1034 | Check Trans Indicator Control-Late MWF/MTW/MX4
F1 | -- | -- | Not Used (L18) | F1 | -- | -- | Not Used (L18)
F1 | WHT | 17 | Stop Lamp Switch Signal (LG5) | F1 | WHT | 17 | Stop Lamp Switch Signal (LG5)
F2 | BRN | 341 | Ignition 3 Voltage | F2 | BRN | 341 | Ignition 3 Voltage
F3 | GRY/BLK | 1467 | Two-Speed Rear Axle Shift Motor Relay Control-All Except MWF/MTW/MX4 | F3 | GRY/BLK | 1467 | Two-Speed Rear Axle Shift Motor Relay Control-All Except MWF/MTW/MX4
F4 | BLK | 150 | Ground | F4 | BLK | 150 | Ground
F6 | PNK | 339 | Ignition 1 Voltage (L18) | F6 | PNK | 339 | Ignition 1 Voltage (L18)
F6 | -- | -- | Not Used (LG5) | F6 | -- | -- | Not Used (LG5)
F7 | -- | -- | Not Used | F7 | -- | -- | Not Used
F8 | BRN | 9 | Park Lamp Supply Voltage | F8 | BRN | 9 | Park Lamp Supply Voltage
F9 | BRN | 441 | Ignition 3 Voltage | F9 | BRN | 441 | Ignition 3 Voltage
G1 | DK BLU | 1944 | Suspension Dump Valve Solenoid Control | G1 | DK BLU | 1944 | Suspension Dump Valve Solenoid Control
G2 | -- | -- | Not Used | G2 | -- | -- | Not Used
G3 | -- | -- | Not Used (L18) | G3 | -- | -- | Not Used (L18)
G3 | GRY | 535 | Coolant Temperature Switch Output (LG5) | G3 | GRY | 535 | Coolant Temperature Switch Output (LG5)
G4 | TAN | 12 | Headlamp Low Beam Supply Voltage | G4 | TAN | 12 | Headlamp Low Beam Supply Voltage
G5 | -- | -- | Not Used (L18) | G5 | -- | -- | Not Used (L18)
G5 | TAN | 848 | Brake Switch Signal (LG5) | G5 | TAN | 848 | Brake Switch Signal (LG5)
G6 | LT GRN | 11 | Headlamp High Beam Supply Voltage | G6 | LT GRN | 11 | Headlamp High Beam Supply Voltage
G7 | DK BLU | 45 | Park Lamp Supply Voltage (RQ3/U86) | G7 | DK BLU | 45 | Park Lamp Supply Voltage (RQ3/U86)
G7 | BRN | 9 | Park Lamp Supply Voltage-All Others | G7 | BRN | 9 | Park Lamp Supply Voltage-All Others
G8 | BRN | 9 | Park Lamp Supply Voltage | G8 | BRN | 9 | Park Lamp Supply Voltage
G9 | BRN | 25 | Charge Indicator Control (L18) | G9 | BRN | 25 | Charge Indicator Control (L18)
G9 | PPL | 1146 | Engine Brake Enable Signal (K40) | G9 | PPL | 1146 | Engine Brake Enable Signal (K40)
G10 | -- | -- | Not Used (L18) | G10 | -- | -- | Not Used (L18)
G10 | PNK | 1905 | Retarder Disable Control (LG5) | G10 | PNK | 1905 | Retarder Disable Control (LG5)

#### C201

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Supply Voltage | A | BRN | 9 | Park Lamp Supply Voltage
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | BLK | 150 | Ground | C | BLK | 150 | Ground
D | ORN | 267 | Heated Mirror Element Feed | D | ORN | 267 | Heated Mirror Element Feed

#### C202

Connector Part Information |

• | 12020397

• | 3 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 2040 | Battery Positive Voltage | A | ORN | 2040 | Battery Positive Voltage-Early LG5
A | ORN | 2040 | Battery Positive Voltage | A | ORN | 2140 | Battery Positive Voltage-L18/Late LG5
B | BLK | 150 | Ground | B | BLK | 150 | Ground
C | PPL | 638 | Power Window Relay-Normally Open Contact | C | PPL | 638 | Power Window Relay-Normally Open Contact

#### C204 (with A/C)

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK BLU | 1199 | Air Temperature Door Control B | A | DK BLU | 1199 | Air Temperature Door Control B
B | YEL | 1318 | Mode Door Control | B | YEL | 1318 | Mode Door Control
C | LT GRN/ BLK | 1647 | Air Inlet Valve Motor Voltage Open | C | LT GRN/ BLK | 1647 | Air Inlet Valve Motor Voltage Open
D | PNK/WHT | 1648 | Air Inlet Valve Motor Voltage Close | D | PNK/WHT | 1648 | Air Inlet Valve Motor Voltage Close
E | LT BLU | 733 | Air Temperature Door Position Signal | E | LT BLU | 733 | Air Temperature Door Position Signal
F | BLK | 470 | Low Reference | F | BLK | 470 | Low Reference
G | YEL/BLK | 1814 | Lower Mode Door Position Sensor Signal | G | YEL/BLK | 1814 | Lower Mode Door Position Sensor Signal
H | GRY | 705 | 5 Volt Reference | H | GRY | 705 | 5 Volt Reference
J | BRN/WHT | 1218 | Upper Mode Valve Motor Supply Voltage | J | BRN/WHT | 1218 | Upper Mode Valve Motor Supply Voltage
K | YEL | 1791 | Air Temperature Door Control A | K | YEL/BLK | 1791 | Air Temperature Door Control A

#### C204 (without A/C)

Connector Part Information |

• | 12092162

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12092163

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 52 | High Blower Control | A | ORN | 52 | High Blower Control
B | BRN | 247 | Blower Enable Relay Control | B | BRN | 247 | Blower Enable Relay Control
C | BLK | 250 | Ground | C | BLK | 250 | Ground
D | GRY | 8 | Instrument Panel Lamp Supply Voltage | D | GRY | 8 | Instrument Panel Lamp Supply Voltage

#### C205

Connector Part Information |

• | 12064762

• | 6 Way F Metri-Pack 150 Series (GRY)

Connector Part Information

• | 12064763

• | 6 Way M Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 199 | Left Rear Speaker Output (+) | A | BRN | 199 | Left Rear Speaker Output (+)
B | WHT | 156 | Courtesy Lamp Low Control | B | WHT | 156 | Courtesy Lamp Low Control
C | DK BLU | 46 | Right Rear Speaker Output (+) | C | DK BLU | 46 | Right Rear Speaker Output (+)
D | LT BLU | 115 | Right Rear Speaker Output (-) | D | LT BLU | 115 | Right Rear Speaker Output (-)
E | ORN | 1040 | Battery Positive Voltage | E | ORN | 1040 | Battery Positive Voltage
F | YEL | 116 | Left Rear Speaker Output (-) | F | YEL | 116 | Left Rear Speaker Output (-)

#### C206

Connector Part Information |

• | 12064752

• | 6 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12064754

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YEL | 318 | Left Rear Trailer Stop/Turn Lamp Supply Voltage | A | YEL | 318 | Left Rear Trailer Stop/Turn Lamp Supply Voltage
B | DK GRN | 319 | Right Rear Trailer Stop/Turn Lamp Supply Voltage | B | DK GRN | 319 | Right Rear Trailer Stop/Turn Lamp Supply Voltage
C | RED | 950 | Trailer Stop Relay-Normally Open Contact | C | RED | 1411 | Trailer Stop Relay-Normally Open Contact
D | DK BLU | 952 | ABS Enable Relay-Normally Open Contact | D | DK BLU | 1413 | ABS Enable Relay-Normally Open Contact
E | BLK | 951 | Park Lamp 3 Supply Voltage | E | BLK | 1412 | Park Lamp 3 Supply Voltage
F | BRN | 9 | Park Lamp Supply Voltage | F | BRN | 9 | Park Lamp Supply Voltage

#### C207

Connector Part Information |

• | 12059884

• | 1 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12059885

• | 1 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | WHT | 22 | Ground | A | WHT | 22 | Ground

#### C208

Connector Part Information |

• | 12047785

• | 4 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047786

• | 4 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Supply Voltage | A | BRN | 9 | Park Lamp Supply Voltage
B | BLK | 250 | Ground | B | BLK | 250 | Ground
C | BLK | 250 | Ground | C | BLK | 250 | Ground
D | ORN | 267 | Heated Mirror Element Feed | C9 | ORN | 267 | Heated Mirror Element Feed

#### C210

Connector Part Information |

• | 12092249

• | 23 Way F Metri-pack 280 Series (BLK)

Connector Part Information

• | 12092248

• | 23 Way M Metri-pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used (L18) | A | -- | -- | Not Used (L18)
A | PNK | 139 | Ignition 1 Voltage (LG5) | A | PNK | 139 | Ignition 1 Voltage (LG5)
B | DK BLU | 527 | Engine Shutdown Alarm Signal (L18) | B | DK BLU | 527 | Engine Shutdown Alarm Signal (L18)
B | LT BLU | 1998 | Intake Air Heater Indicator Control (LG5) | B | LT BLU | 1998 | Intake Air Heater Indicator Control (LG5)
C | GRY | 803 | Change Engine Oil Indicator Control (L18) | C | GRY | 803 | Change Engine Oil Indicator Control (L18)
C | BLK/WHT | 771 | Transmission Range Switch Signal A (MWF) | C | BLK/WHT | 771 | Transmission Range Switch Signal A (MWF)
D | GRY | 397 | Cruise Control On Switch Signal (L18) | D | GRY | 397 | Cruise Control On Switch Signal (L18)
D | GRY | 598 | 5 Volt Reference (MWF) | D | GRY | 598 | 5 Volt Reference (MWF)
E | BRN | 445 | Oil Pressure Gage Signal (L18) | E | BRN | 445 | Oil Pressure Gage Signal (L18)
E | BRN | 841 | Ignition 3 Voltage-Super LG5 | E | BRN | 841 | Ignition 3 Voltage-Super LG5
F | WHT/BLK | 499 | Reduced Engine Power Indicator Control (L18) | F | WHT/BLK | 499 | Reduced Engine Power Indicator Control (L18)
F | YEL | 772 | Transmission Range Switch Signal B (MWF) | F | YEL | 772 | Transmission Range Switch Signal B (MWF)
G | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal (L18) | G | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal (L18)
G | BLK/WHT | 1351 | Ground (MWF) | G | BLK/WHT | 1351 | Ground (MWF)
H | PPL | 806 | Crank Voltage | H | PPL | 806 | Crank Voltage
J | GRY | 120 | Fuel Pump Supply Voltage (L18) | J | GRY | 120 | Fuel Pump Supply Voltage (L18)
J | GRY | 773 | Transmission Range Switch Signal C (MWF) | J | GRY | 773 | Transmission Range Switch Signal C (MWF)
K | DK BLU | 84 | Cruise Control Set/Coast Switch Signal (L18) | K | DK BLU | 84 | Cruise Control Set/Coast Switch Signal (L18)
K | ORN | 1940 | Battery Positive Voltage (MWF) | K | ORN | 1940 | Battery Positive Voltage (MWF)
L | BLK/WHT | 451 | Ground | L | BLK/WHT | 451 | Ground
M | -- | -- | Not Used | M | -- | -- | Not Used
M | LT GRN | 1371 | Transmission Position Switch Signal-Bit 4 (MWF) | M | LT GRN | 1371 | Transmission Position Switch Signal-Bit 4 (MWF)
N | LT GRN | 526 | Stop Lamp Switch Signal (L18) | N | LT GRN | 526 | Stop Lamp Switch Signal (L18)
N | DK BLU | 1378 | Transmission Shift Selector Display Signal (MWF) | N | DK BLU | 1378 | Transmission Shift Selector Display Signal (MWF)
P | DK GRN | 1049 | Class 2 Serial Data (L18) | P | DK GRN | 1049 | Class 2 Serial Data (L18)
P | PNK | 39 | Ignition 1 Voltage (LG5) | P | PNK | 39 | Ignition 1 Voltage (LG5)
R | WHT | 121 | Engine Speed Signal (L18) | R | WHT | 121 | Engine Speed Signal (L18)
R | WHT | 776 | Transmission Range Switch Signal P (MWF) | R | WHT | 776 | Transmission Range Switch Signal P (MWF)
S | YEL/BLK | 68 | Low Coolant Level Indicator Control (L18) | S | YEL/BLK | 68 | Low Coolant Level Indicator Control (L18)
S | BLK/WHT | 1962 | Engine Brake Solenoid Feed (K40) | S | BLK/WHT | 1962 | Engine Brake Solenoid Feed (K40)
T | BRN/WHT | 419 | MIL Control (L18) | T | BRN/WHT | 419 | MIL Control (L18)
T | ORN/BLK | 1786 | Transmission Park/Neutral Signal-All LG5 Except MWF/MTW/MX4 | T | ORN/BLK | 1786 | Transmission Park/Neutral Signal-All LG5 Except MWF/MTW/MX4
U | DK GRN | 465 | Fuel Pump Relay Control (L18) | U | DK GRN | 465 | Fuel Pump Relay Control (L18)
U | -- | -- | Not Used (LG5) | U | -- | -- | Not Used (LG5)
V | LT BLU | 1377 | Check Gages Indicator Control (L18) | V | LT BLU | 1377 | Check Gages Indicator Control (L18)
V | BRN | 25 | Charge Indicator Control (LG5) | V | BRN | 25 | Charge Indicator Control (LG5)
W | DK BLU | 1938 | Engine Overspeed Indicator Control (L18) | W | DK BLU | 1938 | Engine Overspeed Indicator Control (L18)
W | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal-All LG5 Except MWF/MTW/MX4 | W | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal-All LG5 Except MWF/MTW/MX4
X | DK GRN/ WHT | 817 | Vehicle Speed Signal (L18) | X | DK GRN/ WHT | 817 | Vehicle Speed Signal (L18)
X | DK GRN | 1373 | Transmission Shift Selector Mode Signal (MWF) | X | DK GRN | 1373 | Transmission Shift Selector Mode Signal (MWF)
Y | ORN | 40 | Battery Positive Voltage (L18) | Y | ORN | 40 | Battery Positive Voltage (L18)
Y | -- | -- | Not Used (LG5) | Y | -- | -- | Not Used (LG5)
Z | BRN/WHT | 379 | CPP Switch Signal-All Except MWF/MTW/MX4 | Z | BRN/WHT | 379 | CPP Switch Signal-All Except MWF/MTW/MX4

#### C215

Connector Part Information |

• | 12034343

• | 2 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12015271

• | 2 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 240 | Battery Positive Voltage | A | ORN | 240 | Battery Positive Voltage
B | BLK | 250 | Ground | B | BLK | 250 | Ground

#### C218

Connector Part Information |

• | 12020397

• | 3 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 76 | Power Window Relay-Normally Open Contact | A | PPL | 638 | Power Window Relay-Normally Open Contact
B | DK BLU/ WHT | 166 | Power Window Master Switch Right Front Up Signal | B | LT BLU | 166 | Power Window Master Switch Right Front Up Signal
C | TAN | 167 | Power Window Master Switch Right Front Down Signal | C | TAN | 167 | Power Window Master Switch Right Front Down Signal

#### C219

Connector Part Information |

• | 12020397

• | 3 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12020398

• | 3 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 76 | Power Window Relay-Normally Open Contact | A | PPL | 638 | Power Window Relay-Normally Open Contact
B | DK BLU/ WHT | 166 | Power Window Master Switch Right Front Up Signal | B | LT BLU | 166 | Power Window Master Switch Right Front Up Signal
C | TAN | 167 | Power Window Master Switch Right Front Down Signal | C | TAN | 167 | Power Window Master Switch Right Front Down Signal

#### C220

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 250 | Ground | A | BLK | 250 | Ground
B | -- | -- | Not Used | B | -- | -- | Not Used
C | GRY | 8 | Instrument Panel Lamp Supply Voltage | C | GRY | 8 | Instrument Panel Lamp Supply Voltage
D | -- | -- | Not Used (L18) | D | -- | -- | Not Used (L18)
D | ORN/BLK | 1786 | Transmission Parks/Neutral Signal (LG5) | D | ORN/BLK | 1786 | Transmission Parks/Neutral Signal (LG5)
E | -- | -- | Not Used (L18) | E | -- | -- | Not Used (L18)
E | PNK | 39 | Ignition 1 Voltage (LG5) | E | PNK | 39 | Ignition 1 Voltage (LG5)
F-G | -- | -- | Not Used | F-G | -- | -- | Not Used
H | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control | H | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control
J | BRN | 441 | Ignition 3 Voltage | J | BRN | 441 | Ignition 3 Voltage
K | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal | K | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal

#### C221

Connector Part Information |

• | 12015344

• | 6 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12015345

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 60 | Battery Positive Voltage | A | ORN | 2040 | Battery Positive Voltage
B | BLK/WHT | 194 | Door Unlock Control | B | WHT | 194 | Door Unlock Control
C | TAN | 294 | Door Lock Motor Unlock | C | TAN | 294 | Door Lock Motor Unlock
D | GRY | 295 | Door Lock Motor Lock | D | GRY | 295 | Door Lock Motor Lock
E | LT BLU | 195 | Door Lock Control | E | LT BLU | 195 | Door Lock Control
F | BLK | 150 | Ground | F | BLK | 150 | Ground

#### C222

Connector Part Information |

• | 12015344

• | 6 Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12015345

• | 6 Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 60 | Battery Positive Voltage | A | ORN | 2040 | Battery Positive Voltage
B | BLK/WHT | 194 | Door Unlock Control | B | WHT | 194 | Door Unlock Control
C | TAN | 294 | Door Lock Motor Unlock | C | TAN | 294 | Door Lock Motor Unlock
D | GRY | 295 | Door Lock Motor Lock | D | GRY | 295 | Door Lock Motor Lock
E | LT BLU | 195 | Door Lock Control | E | LT BLU | 195 | Door Lock Control
F | -- | -- | Not Used | F | -- | -- | Not Used

#### C223

Connector Part Information |

• | 12064867

• | 2 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064868

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT BLU | 1134 | Park Brake Switch Signal | A | LT BLU | 1134 | Park Brake Switch Signal
B | BLK | 150 | Ground | B | BLK | 150 | Ground

#### C225

Connector Part Information |

• | 12064869

• | 2 Way F Metri-Pack 150 Series (BLU)

Connector Part Information

• | 12064870

• | 2 Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RED | 1673 | 12 Volt Reference (L18) | A | PNK | 39 | Ignition 1 Voltage (L18)
A | RED | 1673 | 12 Volt Reference (LG5) | A | BRN/WHT | 379 | CPP Switch Signal (LG5)
B | RED | 1673 | 12 Volt Reference (L18) | B | BRN/WHT | 379 | CPP Switch Signal (L18)
B | RED | 1673 | 12 Volt Reference (LG5) | B | BLK | 808 | Low Reference (LG5)

#### C226

Connector Part Information |

• | 12052832

• | 2 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12052833

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1140 | Battery Positive Voltage | A | ORN | 1140 | Battery Positive Voltage
B | YEL | 1492 | Park Brake Switch Supply Voltage | B | YEL | 1492 | Park Brake Switch Supply Voltage

#### C227

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY | 48 | CPP Switch Signal | A | GRY | 48 | CPP Switch Signal
B | PPL | 806 | Crank Voltage | B | GRY | 48 | CPP Switch Signal

#### C228

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2 Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage | A | PNK | 39 | Ignition 1 Voltage
B | PNK | 39 | Ignition 1 Voltage | B | PNK | 39 | Ignition 1 Voltage

#### C229

Connector Part Information |

• | 12047662

• | 2 Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12047663

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Supply Voltage | A | BRN | 9 | Park Lamp Supply Voltage
A | BRN | 9 | Park Lamp Supply Voltage | A | DK BLU | 45 | Park Lamp Supply Voltage (RQ3/U86)
B | BLK | 150 | Ground | B | BLK | 150 | Ground

#### C230

Connector Part Information |

• | 12064769

• | 10 Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12064770

• | 10 Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 250 | Ground | A | BLK | 250 | Ground
B | -- | -- | Not Used | B | -- | -- | Not Used
C | GRY | 8 | Instrument Panel Lamp Supply Voltage | C | GRY | 8 | Instrument Panel Lamp Supply Voltage
D | -- | -- | Not Used (L18) | D | -- | -- | Not Used (L18)
D | ORN/BLK | 1786 | Transmission Parks/Neutral Signal (LG5) | D | ORN/BLK | 1786 | Transmission Parks/Neutral Signal (LG5)
E | -- | -- | Not Used (L18) | E | -- | -- | Not Used (L18)
E | PNK | 39 | Ignition 1 Voltage (LG5) | E | PNK | 39 | Ignition 1 Voltage (LG5)
F-G | -- | -- | Not Used | F-G | -- | -- | Not Used
H | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control | H | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control
J | BRN | 441 | Ignition 3 Voltage | J | BRN | 441 | Ignition 3 Voltage
K | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal | K | TAN/WHT | 585 | Transmission Oil Temperature Sensor Signal

#### C403

Connector Part Information |

• | 12040977

• | 3 Way F Metri-Pack 280 Series, Sealed (BLK)

Connector Part Information

• | 1530003

• | 3 Way M Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage | A | BRN | 241 | Ignition 3 Voltage
B | BRN | 341 | Ignition 3 Voltage | B | BRN | 341 | Ignition 3 Voltage
C | BRN | 9 | Park Lamp Supply Voltage | C | BRN | 9 | Park Lamp Supply Voltage

#### C404

Connector Part Information |

• | 12040977

• | 3 Way F Metri-Pack 280 Series, Sealed (BLK)

Connector Part Information

• | 15300003

• | 3 Way M Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage | A | BRN | 241 | Ignition 3 Voltage (RQ2)
A | BRN | 241 | Ignition 3 Voltage | A | BRN | 341 | Ignition 3 Voltage (RQ3)
B | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control | B | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control
C | BLK | 450 | Ground | C | BLK | 450 | Ground

#### C405

Connector Part Information |

• | 12047937

• | 8 Way F Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12047931

• | 8 Way M Metri-Pack 150 (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 9 | Park Lamp Supply Voltage | A | BRN | 9 | Park Lamp Supply Voltage
B | LT GRN | 24 | Backup Lamp Supply Voltage | B | LT GRN | 24 | Backup Lamp Supply Voltage
C | YEL | 18 | Left Rear Stop/Turn Lamp Supply Voltage | C | YEL | 18 | Left Rear Stop/Turn Lamp Supply Voltage
D | DK GRN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | D | DK GRN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
E | GRY | 120 | Fuel Pump Supply Voltage (L18) | E | GRY | 120 | Fuel Pump Supply Voltage (L18)
E | -- | -- | Not Used (LG5) | E | -- | -- | Not Used (LG5)
F | PPL | 30 | Fuel Level Sensor Signal | F | PPL | 30 | Fuel Level Sensor Signal
G | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control | G | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control
H | DK BLU | 1944 | Suspension Dump Valve Solenoid Control | H | DK BLU | 1944 | Suspension Dump Valve Solenoid Control

#### C406

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 341 | Ignition 3 Voltage | A | BRN | 241 | Ignition 3 Voltage (RQ2)
A | BRN | 341 | Ignition 3 Voltage | A | BRN | 341 | Ignition 3 Voltage (RQ3)
B | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control | B | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control

#### C408

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Connector Part Information

• | 12162343

• | 2 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 323 | Shift Solenoid Feed | A | BRN | 323 | Shift Solenoid Feed
B | BLK | 150 | Ground (L18) | B | BLK | 150 | Ground (L18)
B | BLK | 650 | Ground-LG5 without MWF/MTW/MX4 | B | BLK | 650 | Ground-LG5 without MWF/MTW/MX4

#### C409

Connector Part Information |

• | 12047937

• | 8 Way F, Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12047931

• | 8 Way M Metri-Pack 150 Series, (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control | A | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control
B | BRN | 441 | Ignition 3 Voltage | B | BRN | 441 | Ignition 3 Voltage
C | LT GRN | 24 | Backup Lamp Supply Voltage | C | LT GRN | 24 | Backup Lamp Supply Voltage
D | BLK | 150 | Ground (L18) | D | BLK | 150 | Ground (L18)
D | PPL | 806 | Crank Voltage (LG5) | D | PPL | 806 | Crank Voltage (LG5)
E | ORN/BLK | 434 | Neutral Safety Switch Signal | E | ORN/BLK | 434 | Neutral Safety Switch Signal
F | LT GRN/ BLK | 822 | VSS Low Signal | F | LT GRN/ BLK | 822 | VSS Low Signal
G | PPL/WHT | 821 | VSS High Signal | G | PPL/WHT | 821 | VSS High Signal
H | BLK | 150 | Ground (L18) | H | BLK | 150 | Ground (L18)
H | BLK | 650 | Ground (LG5) | H | BLK | 650 | Ground (LG5)

#### C411

Connector Part Information |

• | 12052848

• | 6 Way F Metri-Pack 150 Series, Sealed (BLK)

Connector Part Information

• | 12124107

• | 6 Way M Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 30 | Fuel Level Sensor Signal | A | PPL | 30 | Fuel Level Sensor Signal
B | BRN | 341 | Ignition 3 Voltage | B | BRN | 341 | Ignition 3 Voltage
C | BLK | 350 | Ground | C | BLK | 350 | Ground
D | -- | -- | Not Used | D | -- | -- | Not Used
E | GRY | 120 | Fuel Pump Supply Voltage | E | GRY | 120 | Fuel Pump Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

#### C412

Connector Part Information |

• | 15300027

• | 2 Way F Metri-Pack 280 Series Sealed (BLK)

Connector Part Information

• | 15300002

• | 2 Way M Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 341 | Ignition 3 Voltage | A | BRN | 341 | Ignition 3 Voltage
B | BLK | 150 | Ground | B | BLK | 150 | Ground

#### C419

Connector Part Information |

• | 12110751

• | 7 Way F Metri-Pack 280 Series Sealed (BLK)

Connector Part Information

• | 12110753

• | 7 Way M Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | DK BLU | 952 | ABS Relay-Normally Open Contact | A | DK BLU | 952 | ABS Relay-Normally Open Contact
B | DK GRN | 319 | Right Rear Trailer Stop/Turn Lamp Supply Voltage | B | DK GRN | 319 | Right Rear Trailer Stop/Turn Lamp Supply Voltage
C | RED | 950 | Trailer Stop Relay-Normally Open Contact | C | RED | 950 | Trailer Stop Relay-Normally Open Contact
D | YEL | 318 | Left Rear Trailer Stop/Turn Lamp Supply Voltage | D | YEL | 318 | Left Rear Trailer Stop/Turn Lamp Supply Voltage
E | BLK | 951 | Park Lamp 3 Supply Voltage | E | BLK | 951 | Park Lamp 3 Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used
G | BRN | 9 | Park Lamp Supply Voltage | G | BRN | 9 | Park Lamp Supply Voltage