For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the General Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Suspension General Diagnosis
2 | Verify the vehicle leans or sways in corners. Does the vehicle operate normally? | System OK | Go to Step 3
3 | Inspect the springs for wear or damage. Is the springs worn or damaged? | Go to Step 6 | Go to Step 4
4 | Inspect the stabilizer shaft link pins for wear or damage. Is the stabilizer shaft link pins worn or damaged? | Go to Step 7 | Go to Step 5
5 | Inspect the tires for the correct tire pressure. Is the tire pressure correct? | Go to Step 8 | Go to Step 6
6 | Replace the springs. Did you complete the repair? | Go to Step 9 | --
7 | Replace the stabilizer shaft link pins. Did you complete the repair? | Go to Step 9 | --
8 | Inflate the tires to the correct pressure. Did you complete the repair? | Go to Step 9 | --
9 | Operate the vehicle in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3