For 1990-2009 cars

Table 1: | Accelerator Pedal Position (APP) Sensor
Table 2: | Clutch Pedal Position (CPP) Switch
Table 3: | Clutch Switch
Table 4: | Engine Coolant Temperature (ECT) Switch (UER)
Table 5: | Engine Metal Temperature Switch (KTE)
Table 6: | Engine Oil Pressure (EOP) Switch
Table 7: | Ether Injector Control Valve
Table 8: | FAST IDLE Indicator
Table 9: | FAST IDLE Switch
Table 10: | Fuel Heater
Table 11: | Multifunction Alarm Module C1
Table 12: | Multifunction Alarm Module C2
Table 13: | Park/Neutral Position (PNP) Switch C1, All Automatic Transmissions Except MWF/MTW/MX4
Table 14: | Park/Neutral Position (PNP) Switch C2, All Automatic Transmissions Except MWF/MTW/MX4
Table 15: | Park/Neutral Position (PNP) Switch C3, All Automatic Transmissions Except MWF/MTW/MX4
Table 16: | Park/Neutral Position (PNP) Switch C1 (MTW/MX4)
Table 17: | Park/Neutral Position (PNP) Switch C2 (MTW/MX4)
Table 18: | Powertrain Control Module (PCM)
Table 19: | Stoplamp Switch Interface Module
Table 20: | Upfitter to PTO Connector
Table 21: | Vehicle Speed Sensor (VSS) (MWF)
Table 22: | Vehicle Speed Sensor (VSS) (MTW/MX4)
Table 23: | Vehicle Speed Sensor (VSS) (All Other Automatic Transmissions)
Table 24: | Vehicle Speed Sensor (VSS) (Manual Transmission)

#### Accelerator Pedal Position (APP) Sensor

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN / BLK | 431 | 8 Volt Reference
B | BLK | 808 | Low Reference
C | DK BLU | 417 | TP Sensor Signal

#### Clutch Pedal Position (CPP) Switch

Connector Part Information |

• | 12064870

• | 2-Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 379 | CPP Switch Signal
B | BLK | 808 | Low Reference

#### Clutch Switch

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 48 | CPP Switch Signal
B | PPL | 806 | Crank Voltage

#### Engine Coolant Temperature (ECT) Switch (UER)

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1675 | Check Gages Indicator Control
B | -- | -- | Not Used

#### Engine Metal Temperature Switch (KTE)

Connector Part Information |

• | 12010973

• | 2-Way M Weather Pack (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 434 | Neutral Safety Switch Signal
B | TAN | 1997 | Ether Solenoid Feed

#### Engine Oil Pressure (EOP) Switch

Connector Part Information |

• | 12065299

• | 1-Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 231 | Oil Pressure Switch Signal

#### Ether Injector Control Valve

Connector Part Information |

• | 12040872

• | 2-Way M Weather Pack Connector and Clip (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 1997 | Ether Solenoid Feed
B | BLK | 150 | Ground

#### FAST IDLE Indicator

Connector Part Information |

• | 12059254

• | 2-Way M Metri-Pack 150 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | RED | 2013 | High Idle Indicator Control

#### FAST IDLE Switch

Connector Part Information |

• | 12052833

• | 2-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 534 | High Idle Switch Output
B | BLK | 808 | Low Reference

#### Fuel Heater

Connector Part Information |

• | 15300027

• | 2-Way F Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 841 | Ignition 3 Voltage
B | BLK | 650 | Ground

#### Multifunction Alarm Module C1

Connector Part Information |

• | 12084944

• | 16-Way F Micro-Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | LT BLU / BLK | 1928 | Brake Booster Fluid Flow Switch Signal (JE3)
A2 | YEL | 53 | Generator Fuse Output
A3 | WHT | 17 | Stop Lamp Switch Signal (JE3)
A4 | ORN/BLK | 434 | Neutral Safety Switch Signal
A5 | PNK | 39 | Ignition 1 Voltage
A6 | TAN/WHT | 33 | Brake Warning Indicator Control (JE3)
A7 | TAN/BLK | 231 | Oil Pressure Switch Signal
A8 | BLK | 150 | Ground
B1 | LT GRN | 1478 | Coolant Level Switch Signal
B2 | YEL/BLK | 68 | Low Coolant Level Indicator Control
B3 | YEL/BLK | 1471 | Brake Warning Indicator Supply Voltage 2 (JE3)
B4 | GRY | 847 | Extended Travel Brake Switch Signal (JE3)
B5 | TAN/WHT | 33 | Brake Warning Indicator Control (JE5)
B6 | LT BLU | 1377 | Check Gages Indicator Control
B7 | BRN | 1675 | Check Gages Indicator Control
B8 | ORN | 1740 | Battery Positive Voltage (JE3)

#### Multifunction Alarm Module C2

Connector Part Information |

• | 12064760

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 850 | Ground
B | BLK | 150 | Ground
C | -- | -- | Not Used
D | GRY | 535 | Coolant Temperature Switch Output

#### Park/Neutral Position (PNP) Switch C1, All Automatic Transmissions Except MWF/MTW/MX4

Connector Part Information |

• | 02962793

• | 1-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN / WHT | 1932 | Transmission Shift Select Switch Park Signal

#### Park/Neutral Position (PNP) Switch C2, All Automatic Transmissions Except MWF/MTW/MX4

Connector Part Information |

• | 02973407

• | 2-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN / BLK | 1933 | Transmission Shift Select Switch Park Low Reference
B | -- | -- | Not Used

#### Park/Neutral Position (PNP) Switch C3, All Automatic Transmissions Except MWF/MTW/MX4

Connector Part Information |

• | 12015034

• | 2-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | ORN/BLK | 1786 | Transmission Park/Neutral Signal

#### Park/Neutral Position (PNP) Switch C1 (MTW/MX4)

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | BRN | 441 | Ignition 3 Voltage
D | BLK | 552 | Low Reference
E | PPL | 806 | Crank Voltage
F | LT GRN | 24 | Backup Lamp Supply Voltage
G | ORN/BLK | 434 | Neutral Safety Switch Signal

#### Park/Neutral Position (PNP) Switch C2 (MTW/MX4)

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series, Sealed (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 771 | Transmission Range Switch Signal A
B | GRY | 773 | Transmission Range Switch Signal C
C | WHT | 776 | Transmission Range Switch Signal P
D | YEL | 772 | Transmission Range Switch Signal B

#### Powertrain Control Module (PCM)

Connector Part Information |

• | 12186584

• | 70-Way F 600/700 Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | LT GRN / BLK | 431 | 8 Volt Reference
5 | BLK | 808 | Low Reference
6 | GRY/BLK | 1467 | Two Speed Rear Axle Shift Motor Relay Control -Late LG5 without MTW/MX4
7 | -- | -- | Not Used
8 | TAN/BLK | 1921 | SAE J1708 Serial Data A
9 | WHT/BLK | 1922 | SAE J1708 Serial Data B
10-11 | -- | -- | Not Used
12 | WHT | 1961 | Engine Brake Switch Output-Super Chassis Only
13-16 | -- | -- | Not Used
17 | YEL | 1389 | Vehicle Speed Signal-Early LG5
18-19 | -- | -- | Not Used
20 | GRY | 324 | Shift Relay Coil Supply Voltage-All Except MWF/MTW/MX4
21 | -- | -- | Not Used
22 | BLK | 808 | Low Reference (MWF)
22 | BRN/WHT | 379 | CPP Switch Signal-All Others
23-27 | -- | -- | Not Used
28 | BRN/WHT | 419 | MIL Control
29 | GRY | 535 | Coolant Temperature Switch Output-Late LG5
30 | -- | -- | Not Used
31 | RED | 2013 | High Idle Indicator Control
32 | YEL | 1389 | Vehicle Speed Signal-Early LG5
32 | BRN | 437 | Vehicle Speed Signal-Late LG5 with MTW/MX4
32 | PPL/WHT | 821 | VSS High Signal-Late LG5 without MTW/MX4
33 | LT GRN / BLK | 822 | VSS Low Signal-Late LG5 without MTW/MX4
34 | DK GRN | 2362 | J1939 Data Link- Late LG5 with MTW/MX4
34 | -- | -- | Not Used
35 | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
36 | DK GRN | 389 | Vehicle Speed Signal
37-39 | -- | -- | Not Used
40 | DK GRN | 534 | High Idle Switch Output
41 | -- | -- | Not Used
42 | BLK | 2363 | Reference-Late LG5 with MTW/MX4
43 | -- | -- | Not Used
44 | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
45 | TAN | 848 | Brake Switch Signal
46 | WHT/BLK | 448 | Powertrain Diagnostic Enable
47-49 | -- | -- | Not Used
50 | YEL | 2361 | J1939 Data Link-Late LG5 with MTW/MX4
51 | -- | -- | Not Used
52-53 | ORN | 2240 | Battery Positive Voltage
54-55 | -- | -- | Not Used
56 | DK BLU | 538 | Fast Idle Enable Signal-Remote PTO
57-58 | -- | -- | Not Used
59 | GRY | 397 | Cruise Control On Switch Signal
60-61 | -- | -- | Not Used
62 | PPL | 1995 | Transmission Park/Neutral Signal-Secondary (MWF)
62 | ORN/BLK | 1786 | Transmission Park/Neutral Signal-All Others
63 | -- | -- | Not Used
64 | WHT | 17 | Stoplamp Switch Signal
65 | BLK/WHT | 451 | Ground
66 | DK BLU | 417 | TP Sensor Signal
67 | BLK/WHT | 451 | Ground
68-69 | -- | -- | Not Used
70 | PNK | 139 | Ignition 1 Voltage

#### Stoplamp Switch Interface Module

Connector Part Information |

• | 12004706

• | 6-Way F Edgeboard Connector (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | PNK | 139 | Ignition 1 Voltage
C | BLK | 850 | Ground
D-F | -- | -- | Not Used

#### Upfitter to PTO Connector

Connector Part Information |

• | 12052644

• | 2-Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 538 | Fast Idle Enable Signal-Remote PTO
B | BLK | 808 | Low Reference

#### Vehicle Speed Sensor (VSS) (MWF)

Connector Part Information |

• | 12162194

• | 2 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 400 | VSS High Signal
B | PPL | 401 | VSS High Signal

#### Vehicle Speed Sensor (VSS) (MTW/MX4)

Connector Part Information |

• | 12162193

• | 2 Way F Metri-Pack 150.2 Series, Sealed, P2S (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL/WHT | 821 | VSS High Signal
B | LT GRN/ BLK | 822 | VSS Low Signal

#### Vehicle Speed Sensor (VSS) (All Other Automatic Transmissions)

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL/WHT | 821 | VSS High Signal
B | LT GRN/ BLK | 822 | VSS Low Signal

#### Vehicle Speed Sensor (VSS) (Manual Transmission)

Connector Part Information |

• | 12162194

• | 2 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL/WHT | 821 | VSS High Signal
B | LT GRN/ BLK | 822 | VSS Low Signal