For 1990-2009 cars

Application | Front Runout | Center Runout | Rear Runout | Stub Shaft Runout
--- | --- | --- | --- | ---
Metric | English | Metric | English | Metric | English | Metric | English
One-Piece Propeller Shafts | 1.016 mm | 0.040 in | 1.27 mm | 0.050 in | 1.40 mm | 0.055 in | -- | --
Two-Piece Propeller Shafts | 0.762 mm | 0.030 in | 0.762 mm | 0.030 in | 0.889 mm | 0.035 in | -- | --
Two-Piece Propeller Shafts Tandem | 0.762 mm ¹ | 0.030 in ¹ | 0.762 mm ¹ | 0.030 in ¹ | 0.889 mm ¹ | 0.035 in ¹ | -- | --
Three-Piece Propeller Shafts | 1.016 mm | 0.040 in | 1.27 mm | 0.050 in | 1.40 mm | 0.055 in | -- | --
¹ Application (First and Second)