For 1990-2009 cars

### Removal Procedure

1. Apply the parking brake.
2. Remove the MaxiFuse® block (1) cover.

Pull down on the parking brake relay (3) in order to remove the parking brake relay (3) from the bracket.

3. Remove the parking brake relay electrical connector (2).

### Installation Procedure

1. Install the parking brake relay electrical connector (2).
2. Install the parking brake relay (3) to the bracket.
3. Install the MaxiFuse® block (1) cover.