For 1990-2009 cars

Cause | Action
--- | ---
DEFINITION: The clutch requires constant adjustment. Review the Symptoms - Clutch and perform the necessary inspections.
Release bearing locknut incorrectly tightened | Adjust the release bearing length per the procedure and tighten to the proper specifications. Refer to Clutch Assembly Adjustment .
Insufficient gap at release yoke to release bearing |

1. Adjust the release bearing length per the procedure and tighten to the proper specifications. Refer to Clutch Assembly Adjustment .
2. Adjust the clutch linkage for the proper gap. Refer to Clutch Assembly Adjustment .

Excessive clutch slippage | Refer to Clutch Slipping .
Clutch wearing excessively |

• | Review the vehicle application.

• | Review the driver practices.