For 1990-2009 cars

Table 1: | Accelerator Pedal Position (APP) Sensor
Table 2: | Camshaft Position (CMP) Sensor
Table 3: | Clutch Pedal Position (CPP) Switch
Table 4: | Clutch Switch
Table 5: | Crankshaft Position (CKP) Sensor
Table 6: | Engine Coolant Temperature (ECT) Sensor
Table 7: | Engine Oil Pressure (EOP) Sensor
Table 8: | Evaporative Emission (EVAP) Canister Purge Solenoid
Table 9: | FAST IDLE Indicator
Table 10: | FAST IDLE Switch
Table 11: | Fuel Pump and Sender Assembly
Table 12: | Fuel Sender and Balance Pump Control Module
Table 13: | Fuel Sender and Balance Pump Control Relay
Table 14: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1
Table 15: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1
Table 16: | Ignition Coils
Table 17: | Ignition Relay -- Engine Controls
Table 18: | Manifold Absolute Pressure (MAP) Sensor
Table 19: | Mass Air Flow (MAF) Sensor
Table 20: | Multifunction Alarm Module
Table 21: | Multiport Fuel Injectors
Table 22: | Neutral Safety Switch
Table 23: | Park/Neutral Position (PNP) Switch C1
Table 24: | Park/Neutral Position (PNP) Switch C2
Table 25: | PTO Switch
Table 26: | Stop Lamp Switch Interface Module
Table 27: | Throttle Actuator Control (TAC) Module C1
Table 28: | Throttle Actuator Control (TAC) Module C2
Table 29: | Throttle Actuator Control (TAC) Motor
Table 30: | Throttle Position (TP) Sensor
Table 31: | Upfitter Power Takeoff Connector
Table 32: | Vehicle Speed Sensor (VSS) -- Automatic Transmission
Table 33: | Vehicle Speed Sensor (VSS) -- Manual Transmission

#### Accelerator Pedal Position (APP) Sensor

Connector Part Information |

• | 12177081

• | 10 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1271 | Low Reference
B | PPL | 1272 | Low Reference
C | LT BLU | 1162 | APP Sensor 2 Signal
D | TAN | 1274 | 5 Volt Reference
E | YEL/BLK | 1275 | 5 Volt Reference
F | DK BLU | 1161 | APP Sensor 1 Signal
G | WHT/BLK | 1164 | 5 Volt Reference
H | -- | -- | Not Used
J | GRY | 1273 | Low Reference
K | DK GRN | 1163 | APP Sensor 3 Signal

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12059595

• | 3 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 631 | 12 Volt Reference
B | PNK/BLK | 632 | Low Reference
C | BRN/WHT | 633 | CMP Sensor Signal

#### Clutch Pedal Position (CPP) Switch

Connector Part Information |

• | 12064870

• | 2 Way M Metri-Pack 150 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | BRN/WHT | 379 | CPP Switch Signal

#### Clutch Switch

Connector Part Information |

• | 12064749

• | 2 Way F Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 48 | CPP Switch Signal
B | PPL | 806 | Crank Voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12059595

• | 3 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1867 | 12 Volt Reference
B | YEL/BLK | 1868 | Low Reference
C | DK BLU/WHT | 1869 | CKP Sensor Signal

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12110293

• | 3 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 720 | Low Reference
B | YEL | 410 | ECT Sensor Signal
C | DK GRN | 135 | Coolant Temperature Sensor Signal

#### Engine Oil Pressure (EOP) Sensor

Connector Part Information |

• | 12078090

• | 3 Way F Metri-Pack 150 Series, Sealed P2S (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 407 | Low Reference
B | GRY | 705 | 5 Volt Reference
C | TAN/WHT | 332 | Oil Pressure Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid

Connector Part Information |

• | 12052643

• | 2 Way F Metri-Pack 150 Series, Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 339 | Ignition 1 Voltage
B | DK GRN/WHT | 428 | EVAP Canister Purge Solenoid Control

#### FAST IDLE Indicator

Connector Part Information |

• | 12059254

• | 2 Way M, Metri-Pack 150 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | RED | 2013 | High Idle Indicator Control

#### FAST IDLE Switch

Connector Part Information |

• | 12052833

• | 2 Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN | 534 | High Idle Switch Output
B | BLK/WHT | 451 | Ground

#### Fuel Pump and Sender Assembly

Connector Part Information |

• | 12162188

• | 4 Way F, Metri-Pack 150 Series, Sealed, (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 350 | Ground
B | -- | -- | Not Used
C | GRY | 120 | Fuel Pump Motor Feed
C | RED | 458 | Fuel Pump Relay Output-Normally Open Contact - Right Fuel Tank
D | DK BLU | 1936 | Fuel Gage Sensor Signal-Left - Left Fuel Tank
D | LT BLU | 1937 | Fuel Gauge Sensor Signal-Right - Right Fuel Tank
D | PPL | 30 | Fuel Level Sensor Signal - Single Fuel Tank

#### Fuel Sender and Balance Pump Control Module

Connector Part Information |

• | 12059573

• | 6 Way F Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 341 | Ignition 3 Voltage
B | LT BLU | 1937 | Fuel Level Sensor Signal-Right
C | DK BLU | 1936 | Fuel Level Sensor Signal-Left
D | LT GRN | 497 | Fuel Pump Relay Control
E | BLK | 350 | Ground
F | PPL | 30 | Fuel Level Sensor Signal

#### Fuel Sender and Balance Pump Control Relay

Connector Part Information |

• | 12129716

• | 4 Way F, Metri-Pack 280 Series, Flexlock, Sealed, (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | BRN | 341 | Ignition 3 Voltage
85 | GRY | 120 | Fuel Pump Supply Voltage
86 | LT GRN | 497 | Fuel Pump Relay Control
87 | RED | 458 | Fuel Pump Relay Output-Normally Open Contact

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1

Connector Part Information |

• | 12092840

• | 5 Way M Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | HO2S Low Signal
B | PPL/WHT | 1665 | HO2S High Signal
C | -- | -- | Not Used
D | LT GRN/WHT | 3213 | Heater Power
E | LT GRN | 3212 | Heater Ground

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1

Connector Part Information |

• | 12146046

• | 5 Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | HO2S Low Signal
B | PPL | 1666 | HO2S High Signal
C | -- | -- | Not Used
D | LT GRN/WHT | 3213 | Heater Power
E | LT GRN | 3212 | Heater Ground

#### Ignition Coils

Connector Part Information |

• | 12162144

• | 4 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 650 | Ground
B | BRN | 2129 | Low Reference - Bank 1-Left
B | BRN | 2130 | Low Reference - Bank 2-Right
C | PPL | 2121 | IC 1 Control - Ignition Coil 1
C | RED | 2122 | IC 2 Control - Ignition Coil 2
C | LT BLU | 2123 | IC 3 Control - Ignition Coil 3
C | DK GRN | 2124 | IC 4 Control - Ignition Coil 4
C | DK GRN | 2125 | IC 5 Control - Ignition Coil 5
C | LT BLU | 2126 | IC 6 Control - Ignition Coil 6
C | RED | 2127 | IC 7 Control - Ignition Coil 7
C | PPL | 2128 | IC 8 Control - Ignition Coil 8
D | PNK | 139 | Ignition 1 Voltage - Bank 1-Left
D | PNK | 239 | Ignition 1 Voltage - Bank 2-Right

#### Ignition Relay -- Engine Controls

Connector Part Information |

• | 12124169

• | 4 Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | RED | 42 | Battery Positive Voltage
85 | PNK | 39 | Ignition 1 Voltage
86 | BLK | 150 | Ground
87 | PPL | 2000 | Ignition 1 Relay Output-Normally Open Contact

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12129946

• | 3 Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | LT GRN | 432 | MAP Sensor Signal
C | GRY | 597 | 5 Volt Reference

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 15305555

• | 5 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 552 | Low Reference
B | TAN | 472 | IAT Sensor Signal
C | BLK/WHT | 451 | Ground
D | PNK | 339 | Ignition 1 Voltage
E | YEL | 492 | MAF Sensor Signal

#### Multifunction Alarm Module

Connector Part Information |

• | 12110259

• | 16 Way F Micro-Pack 100 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | LT BLU | 1377 | Check Gages Indicator Control
A3 | LT GRN | 1478 | Coolant Level Switch Signal
A4 | LT BLU/BLK | 1928 | Brake Booster Fluid Flow Switch Signal (JE3)
A4 | -- | -- | Not Used (JE5)
A5 | GRY | 847 | Extended Travel Brake Switch Signal (JE3)
A5 | -- | -- | Not Used (JE5)
A6 | PNK | 39 | Ignition 1 Voltage
A7 | WHT | 17 | Stop Lamp Switch Signal (JE3)
A7 | -- | -- | Not Used (JE5)
A8 | ORN | 1740 | Battery Positive Voltage (JE3)
A8 | -- | -- | Not Used (JE5)
B1 | YEL/BLK | 68 | Low Coolant Level Indicator Control
B2 | TAN/WHT | 33 | Brake Warning Indicator Control (JE3)
B2 | -- | -- | Not Used (JE5)
B3 | YEL/BLK | 1471 | Brake Warning Indicator Supply Voltage 2 (JE3)
B3 | -- | -- | Not Used (JE5)
B4 | BLK | 150 | Ground
B5 | -- | -- | Not Used (JE3)
B5 | TAN/WHT | 33 | Brake Warning Indicator Control (JE5)
B6 | PPL | 806 | Crank Voltage
B7 | YEL | 53 | Fuse Output-Generator-Tachometer Pulse
B8 | DK BLU | 527 | Engine Shutdown Alarm Signal

#### Multiport Fuel Injectors

Connector Part Information |

• | 15326181

• | 2 Way F Micro-Pack Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 139 | Ignition 1 Voltage (Bank 1-Left)
A | PNK | 139 | Ignition 1 Voltage - Bank 2-Right
B | BLK | 1744 | Fuel Injector 1 Control - Multiport Fuel Injector 1
B | LT GRN/BLK | 1745 | Fuel Injector 2 Control - Multiport Fuel Injector 2
B | PNK/BLK | 1746 | Fuel Injector 3 Control - Multiport Fuel Injector 3
B | LT BLU/BLK | 844 | Fuel Injector 4 Control - Multiport Fuel Injector 4
B | BLK/WHT | 845 | Fuel Injector 5 Control - Multiport Fuel Injector 5
B | YEL/BLK | 846 | Fuel Injector 6 Control - Multiport Fuel Injector 6
B | RED/BLK | 877 | Fuel Injector 7 Control - Multiport Fuel Injector 7
B | DK BLU/WHT | 878 | Fuel Injector 8 Control - Multiport Fuel Injector 8

#### Neutral Safety Switch

Connector Part Information |

• | 12124819

• | 2 Way F Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 806 | Crank Voltage
B | ORN/BLK | 434 | Neutral Safety Switch Signal

#### Park/Neutral Position (PNP) Switch C1

Connector Part Information |

• | 02962793

• | 1 Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK GRN/WHT | 1932 | Transmission Shift Select Switch - Park Signal

#### Park/Neutral Position (PNP) Switch C2

Connector Part Information |

• | 02973407

• | 2 Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 1933 | Transmission Shift Select Switch - Park Low Reference
B | -- | -- | Not Used

#### PTO Switch

Connector Part Information |

• | 12047782

• | 3 Way M Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | LT GRN | 488 | PTO Enable Switch Input
C | BLK/WHT | 451 | PCM Ground

#### Stop Lamp Switch Interface Module

Connector Part Information |

• | 12004706

• | 6 Way Edgeboard Series, Standard (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 39 | Ignition 1 Voltage
B | PPL | 420 | TCC Brake Switch Signal
C | TAN | 848 | Brake Switch Signal
D | WHT | 17 | Stop Lamp Switch Signal
E | BLK/WHT | 451 | Ground
F | LT GRN | 526 | Stop Lamp Switch Signal

#### Throttle Actuator Control (TAC) Module C1

Connector Part Information |

• | 12177081

• | 10 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1271 | Low Reference
B | PPL | 1272 | Low Reference
C | LT BLU | 1162 | APP Sensor 2 Signal
D | TAN | 1274 | 5 Volt Reference
E | YEL/BLK | 1275 | 5 Volt Reference
F | DK BLU | 1161 | APP Sensor 1 Signal
G | WHT/BLK | 1164 | 5 Volt Reference
H | -- | -- | Not Used
J | GRY | 1273 | Low Reference
K | DK GRN | 1163 | APP Sensor 3 Signal

#### Throttle Actuator Control (TAC) Module C2

Connector Part Information |

• | 12191065

• | 16 Way F Micro-Pack 100W Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | DK GRN | 485 | TP Sensor 1 Signal
2 | GRY | 416 | 5 Volt Reference
3 | BRN | 452 | Low Reference
4 | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
5 | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
6 | LT GRN | 526 | Stop Lamp Switch Signal
7 | PNK | 339 | Ignition 1 Voltage
8 | BRN | 582 | TAC Motor Control-2
9 | LT BLU/BLK | 1688 | 5 Volt Reference
10 | BLK/WHT | 1704 | Low Reference
11 | PPL | 486 | TP Sensor 2 Signal
12 | ORN/BLK | 1061 | UART Serial Data - Secondary
13 | DK BLU/WHT | 774 | UART Serial Data - Tertiary
14 | GRY | 397 | Cruise Control On Switch Signal
15 | BLK/WHT | 451 | Ground
16 | YEL | 581 | TAC Motor Control-1

#### Throttle Actuator Control (TAC) Motor

Connector Part Information |

• | 12077900

• | 2 Way F Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 582 | TAC Motor Control-2
B | YEL | 581 | TAC Motor Control-1

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12162260

• | 6 Way F Metri-Pack 150.2 Series, Sealed P2S (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 416 | 5 Volt Reference
B | BLK | 452 | Low Reference
C | DK GRN | 485 | TP Sensor 1 Signal
D | LT BLU/BLK | 1688 | 5 Volt Reference
E | BLK/WHT | 1704 | Low Reference
F | PPL | 486 | TP Sensor 2 Signal

#### Upfitter Power Takeoff Connector

Connector Part Information |

• | 12047937

• | 8 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 451 | Ground
B | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
C | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
D | LT GRN | 488 | PTO Enable Switch Input
E | -- | -- | Not Used
F | PPL | 2562 | PTO Relay Output-Coil
G | -- | -- | Not Used
H | LT BLU | 494 | PTO Switch Output

#### Vehicle Speed Sensor (VSS) -- Automatic Transmission

Connector Part Information |

• | 12052644

• | 2 Way F Metri-Pack 150 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL/WHT | 821 | VSS High Signal
B | LT GRN/BLK | 822 | VSS Low Signal

#### Vehicle Speed Sensor (VSS) -- Manual Transmission

Connector Part Information |

• | 12162194

• | 2 Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL/WHT | 821 | VSS High Signal
B | LT GRN/BLK | 822 | VSS Low Signal