For 1990-2009 cars

Causes | Action
--- | ---
DEFINITION: Growl or whine noise from the clutch when engaged or disengaged. Review the Symptoms - Clutch and perform the necessary inspections.
The pilot bearing is worn or damaged | Replace the pilot bearing. Refer to Clutch Assembly Replacement .
The clutch cable is binding | Replace the clutch cable. Refer to Clutch Cable Replacement .
The clutch cable is contacting the cab or frame | Repair the cable to prevent it from causing a noise.
Incorrect release bearing bore size for the clutch application | Replace the release bearing. Refer to Release Bearing Replacement .
The release bearing is worn or damaged | Replace the release bearing. Refer to Release Bearing Replacement .