For 1990-2009 cars

Figure 1: |

#### Center of the I/P

(1) | Driver Information Systems Connectors
(2) | Radio Connectors
(3) | Auxiliary Power Post
(4) | Auxiliary Power Post
(5) | HVAC Control Connector
(6) | HVAC Control Connector

Figure 2: |

#### Front Left of the I/P

(1) | Radio
(2) | Park Brake Release Switch
(3) | HVAC Control Module
(4) | Overdrive Defeat Switch
(5) | Headlamp Switch
(6) | Instrument Panel Cluster

Figure 3: |

#### Left Front Door

(1) | Door Lock Switch - Driver (AU3)
(2) | Outside Rearview Mirror Switch (DB6)
(3) | Window Switch - Driver (A31)
(4) | Outside Rearview Mirror Switch Connector
(5) | Window Switch - Driver Connector
(6) | Door Lock Switch - Driver Connector
(7) | Speaker - LF Tweeter Connector
(8) | Speaker - LF Tweeter (ZQ2)
(9) | Speaker - LF
(10) | Speaker - LF Connector
(11) | Window Motor - Driver (A31)
(12) | Door Latch Assembly - Driver C1 (Lock Actuator)
(13) | Door Latch Assembly - Driver C2 (Jamb Switch)

Figure 4: |

#### Left Rear Door (Crew Cab)

(1) | Speaker - LR
(2) | Window Switch - LR
(3) | C301 (12 cavities - Crew Cab)
(4) | Window Motor - LR
(5) | Door Latch Assembly - LR

Figure 5: |

#### Right Front Door

(1) | Door Lock Switch - Passenger (AU3)
(2) | Window Switch - Passenger (A31)
(3) | Window Switch - Passenger Connector
(4) | Door Lock Switch - Passenger Connector
(5) | Speaker - RF Tweeter Connector
(6) | Speaker - RF Tweeter (ZQ2)
(7) | Door Latch Assembly - Passenger C1 (Lock Actuator)
(8) | Door Latch Assembly - Passenger C2 (Jamb Switch)
(9) | Window Motor - Passenger (A31)
(10) | Speaker - RF Connector
(11) | Speaker - RF

Figure 6: |

#### Right Rear Door (Crew Cab)

(1) | Window Switch - RR
(2) | Speaker - RR
(3) | Door Latch Assembly - RR
(4) | Window Motor - RR
(5) | C302 (12 Cavities - Crew Cab)