For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Radio/Audio System Schematics
1 | Did you review the Radio/Audio Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Radio/Audio System Description and Operation
2 | Use the J 39916-A CD and Cassette Diagnostic Audio Kit in order to perform the motor speed test. Is the cassette motor speed correct? | Go to Step 3 | Go to Step 4
3 | Use the J 39916-A CD in order to clean the cassette player. Did you complete the repair? | Go to Step 5 | --
4 | Important:: Perform the set up procedure for the radio. Replace the radio. Refer to Radio Replacement . Did you complete the repair? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2