For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air compressor bracket front bracket bolt-front of engine | 64 N·m | 47 lb in
Air compressor bracket front bracket bolt-side of engine | 54 N·m | 40 lb in
Air Compressor Crankshaft Gear Nut | 160 N·m | 118 lb ft
Air Compressor Mounting Bracket Bolt | 67 N·m | 49 lb ft
Air Compressor Mounting Bracket to Engine Bolt | 67 N·m | 49 lb ft
Air Compressor Mounting Flange Bolt | 100 N·m | 74 lb ft
Air compressor pulley nut | 140 N·m | 103 lb in
Air Inlet Hose Clamp | 2.75 N·m | 24 lb in
Coolant Inlet Hose Nut | 24 N·m | 18 lb ft
Coolant Outlet Hose Nut | 24 N·m | 18 lb ft
Discharge Line Nut | 22 N·m | 16 lb ft
Governor Mounting Bolt | 21 N·m | 15 lb ft
Oil Supply Hose Clip Bolt | 67 N·m | 49 lb ft
Oil Supply Hose Nut | 13 N·m | 115 lb in