For 1990-2009 cars

### Removal Procedure

1. Block the wheels.
2. Remove the pin from the parking brake switch knob.
3. Remove the parking brake switch knob.
4. Remove the parking brake switch mounting nut.
5. Remove the parking brake switch mounting washer.
6. Remove the parking brake switch.
7. Remove the parking brake switch electrical connector.

### Installation Procedure

1. Install the parking brake switch electrical connector.
2. Install the parking brake switch.
3. Install the parking brake switch mounting washer.
4. Install the parking brake switch mounting nut.
5. Install the parking brake switch knob.
6. Ensure that the lettering on the knob is facing the correct way.
7. Install the pin to the parking brake switch knob.
8. Remove the wheel blocks.