For 1990-2009 cars

Table 1: | Ashtray Lamp
Table 2: | Backup Lamp Switch
Table 3: | Clearance Lamps
Table 4: | Daytime Running Lamps (DRL) Control Module
Table 5: | Daytime Running Lamps (DRL) Diode
Table 6: | Door Jamb Switch -- Driver
Table 7: | Hazard Indicator Lamp
Table 8: | Hazard Switch
Table 9: | Headlamp Dimmer Switch
Table 10: | Headlamp Switch
Table 11: | Headlamps
Table 12: | Heater Control Lamps
Table 13: | IP Dimmer Switch
Table 14: | Marker Lamps -- Roof
Table 15: | Park/Turn Signal Lamps
Table 16: | Park Brake Switch (JE5)
Table 17: | Stop Lamp Relay 1
Table 18: | Stop Lamp Relay 2
Table 19: | Stop Lamp Switch C1
Table 20: | Stop Lamp Switch C2
Table 21: | Tail Lamps
Table 22: | Tractor/Trailer Receptacle
Table 23: | Trailer Marker Lamp Switch
Table 24: | Trailer Stop Lamp Relay
Table 25: | Trailer Stop Lamp Switch
Table 26: | Turn Signal/Hazard Flasher Module
Table 27: | Turn Signal Switch/Multifunction Switch C1

#### Ashtray Lamp

Connector Part Information |

• | 12124722

• | 2-Way Type W2 Axial (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 250 | Ground
B | GRY | 8 | Instrument Panel Lamp Supply Voltage

#### Backup Lamp Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 441 | Ignition 3 Voltage
B | LT GRN | 24 | Backup Lamp Supply Voltage

#### Clearance Lamps

Connector Part Information |

• | 06294702

• | Bulb Base Type W-2, (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Lamp Supply Voltage
B | BLK | 150 | Ground

#### Daytime Running Lamps (DRL) Control Module

Connector Part Information |

• | 12191131

• | 8-Way F Printed Circuit Connector Edgeboard Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 1134 | Park Brake Switch Signal
B | -- | -- | Not Used
C | PNK | 39 | Ignition 1 Voltage
D | YEL | 10 | Headlamp Switch Signal
E-F | -- | -- | Not Used
G | LT GRN/ BLK | 592 | DRL Relay Control
H | BLK | 250 | Ground

#### Daytime Running Lamps (DRL) Diode

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 634 | DRL Diode Supply Voltage
B | WHT | 815 | DRL Diode Signal

#### Door Jamb Switch -- Driver

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 156 | Courtesy Lamp Low Control
B | BLK | 150 | Ground
C | -- | -- | Not Used

#### Hazard Indicator Lamp

Connector Part Information |

• | 12047663

• | 2-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Supply Voltage
B | BLK | 150 | Ground

#### Hazard Switch

Connector Part Information |

• | 12034482

• | 6-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 27 | Hazard Flasher Signal
B | YEL | 18 | Left Rear Stop/Turn Lamp Supply Voltage
C | DK BLU | 15 | Right Turn Signal Lamps Supply Voltage
D | DK GRN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
E | LT BLU | 14 | Left Turn Signal Lamps Supply Voltage
F | BLK | 150 | Ground

#### Headlamp Dimmer Switch

Connector Part Information |

• | 08917693

• | 4-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 11 | Headlamp High Beam Supply Voltage
B | -- | -- | Not Used
C | PPL | 544 | DRL Relay Contact-Normally Closed
D | YEL | 10 | Headlamp Switch Signal

#### Headlamp Switch

Connector Part Information |

• | 12034061

• | 6-Way F Metri-Pack 480 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 13 | Headlamp Switch Park Lamps Signal
B | YEL | 634 | DRL Diode Supply Voltage
C | RED | 1042 | Battery Positive Voltage
D | YEL | 10 | Headlamp Switch Signal
E | ORN | 1040 | Battery Positive Voltage
F | -- | -- | Not Used

#### Headlamps

Connector Part Information |

• | 12034372

• | 3-Way F Metri-Pack 800 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 150 | Ground
B | LT GRN | 11 | Headlamp High Beam Supply Voltage
C | TAN | 12 | Headlamp Low Beam Supply Voltage

#### Heater Control Lamps

Connector Part Information |

• | 12110566

• | Bulb Base Type W-1 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Supply Voltage
B | BLK | 250 | Ground

#### IP Dimmer Switch

Connector Part Information |

• | 12034060

• | 4-Way F Metri-Pack 480 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 13 | Headlamp Switch Park Lamps Signal
B | BLK | 150 | Ground
C | WHT | 156 | Courtesy Lamp Low Control
D | GRY | 8 | Instrument Panel Lamp Supply Voltage

#### Marker Lamps -- Roof

Connector Part Information |

• | 06294702

• | Bulb Base Type W-2 (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Lamp Supply Voltage
B | BLK | 150 | Ground

#### Park/Turn Signal Lamps

Connector Part Information |

• | 12162185

• | 3-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 14 | Turn Signal Lamps Supply Voltage - Left Front
A | DK BLU | 15 | Turn Signal Lamps Supply Voltage - Right Front
B | BLK | 150 | Ground
C | BRN | 9 | Park Lamps Supply Voltage

#### Park Brake Switch (JE5)

Connector Part Information |

• | 12065298

• | 4-Way F Metri-Pack 150 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 1134 | Park Brake Switch Signal
B | BLK | 150 | Ground
C-D | -- | -- | Not Used

#### Stop Lamp Relay 1

Connector Part Information |

• | 12110541

• | 6-Way F, Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BLK | 250 | Ground
A2 | LT BLU | 20 | Stop Lamp Supply Voltage
B1-B2 | -- | -- | Not Used
C1 | ORN | 1240 | Battery Positive Voltage
C2 | WHT | 17 | Stop Lamp Switch Signal

#### Stop Lamp Relay 2

Connector Part Information |

• | 12129715

• | 6-Way F Metri-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | BLK | 250 | Ground
A2 | LT BLU | 20 | Stop Lamp Supply Voltage
B1-B2 | -- | -- | Not Used
C1 | ORN | 1240 | Battery Positive Voltage
C2 | WHT | 17 | Stop Lamp Switch Signal

#### Stop Lamp Switch C1

Connector Part Information |

• | 12033704

• | 4-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1240 | Battery Positive Voltage
B | WHT | 17 | Stop Lamp Switch Signal
C | ORN | 540 | Battery Positive Voltage
D | GRY | 847 | Extended Travel Brake Switch Signal

#### Stop Lamp Switch C2

Connector Part Information |

• | 12033709

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 848 | Brake Switch Signal
B | BLK/WHT | 451 | Ground

#### Tail Lamps

Connector Part Information |

• | 12065862

• | 4-Way F Metri-Pack 280 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 24 | Backup Lamp Supply Voltage
B | BRN | 9 | Park Lamp Supply Voltage
C | YEL | 18 | Rear Stop/Turn Lamp Supply Voltage - Left
C | DK GRN | 19 | Rear Stop/Turn Lamp Supply Voltage - Right
E | BLK | 150 | Ground

#### Tractor/Trailer Receptacle

Connector Part Information |

• | 12077629

• | 7-Way M Split Terminal Connector (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 22 | Ground
B | BLK | 951 | Tractor Marker Lamps Relay
C | YEL | 318 | Left Rear Trailer Stop/Turn Lamp Supply Voltage
D | RED | 950 | Trailer Stop Lamps Relay
E | DK GRN | 319 | Right Rear Trailer Stop/Turn Lamp Supply Voltage
F | BRN | 9 | Park Lamp Supply Voltage
G | DK BLU | 952 | Air ABS Relay

#### Trailer Marker Lamp Switch

Connector Part Information |

• | 12052054

• | 4-Way M Metri-Pack 150 Series, (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Supply Voltage
B | ORN | 840 | Battery Positive Voltage
C | DK GRN | 21 | Roof Clearance Lamps Switch Signal
D | BLK | 250 | Ground

#### Trailer Stop Lamp Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | RED | 1442 | Battery Positive Voltage
85 | WHT | 17 | Stop Lamp Switch Signal
86 | BLK | 150 | Ground
87 | RED | 1411 | Trailer Stop Relay-Normally Open Contact

#### Trailer Stop Lamp Switch

Connector Part Information |

• | 12065402

• | 4-Way F Metri-Pack 150 Series, Sealed (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used-Sealed
C | ORN | 1240 | Battery Positive Voltage
D | WHT | 17 | Stop Lamp Switch Signal

#### Turn Signal/Hazard Flasher Module

Connector Part Information |

• | 12103751

• | 5-Way F Metri-Pack 630 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | ORN | 1540 | Battery Positive Voltage
3 | -- | -- | Not Used
4 | PPL | 16 | Turn Signal Flasher Signal
4 | BRN | 27 | Hazard Flasher Signal
5 | BLK | 150 | Ground

#### Turn Signal Switch/Multifunction Switch C1

Connector Part Information |

• | 12004147

• | 11-Way F Pack-Con Series 1 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
D | GRY | 8 | Instrument Panel Lamp Supply Voltage
E-F | -- | -- | Not Used
G | BLK | 28 | Horn Relay Control
H | LT BLU | 14 | Left Turn Signal Lamps Supply Voltage
J | DK BLU | 15 | Right Turn Signal Lamps Supply Voltage
K | BRN | 27 | Hazard Flasher Signal
L | PPL | 16 | Turn Signal Flasher Signal
M | YEL | 18 | Left Rear Stop/Turn Lamp Supply Voltage
N | DK GRN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
P | LT BLU | 20 | Stop Lamp Supply Voltage