For 1990-2009 cars

#### Tire Wear

(1) | Hard Cornering/Underinflation
(2) | Incorrect Alignment/Lack of Rotation
(3) | Incorrect Alignment/Non-uniform Tire
(4) | Over Inflation
(5) | Wear Indicator

Inspect the tire and wheel assemblies for the following conditions:

• | Unusual wear such as cupping, flat spots, and/or heel-and-toe wear

| (These conditions can cause tire growl, tire howl, slapping noises, and/or vibrations throughout the vehicle.)

• | Proper inflation (to specifications for the vehicle)

• | Bulges in the sidewalls

| (Do not confuse bulges, which are an abnormal condition, with normal ply splices which are commonly seen as indentations in the sidewall.)

• | Bent rim flanges