For 1990-2009 cars

Causes | Action
--- | ---
DEFINITION: A rattle noise coming from the clutch components with the clutch disengaged or engaged. Review the Symptoms - Clutch and perform the necessary inspections.
The linkage needs adjustment | Adjust the clutch linkage.
The linkage is worn | Repair or replace as necessary.
The linkage needs lubrication | Perform lubrication maintenance on the linkage.
Clutch brake rattle | Replace the clutch brake. Refer to Clutch Brake Replacement .
Idle rattle clutch engaged | Replace the clutch disc, due to faulty damper springs. Refer to Clutch Assembly Replacement .
The clutch is improperly installed | Remove the clutch and reinstall it correctly. Refer to Clutch Assembly Replacement .
The clutch disc damper worn or damaged | Inspect the clutch disc for a broken or worn damper. Replace the clutch assembly. Refer to Clutch Assembly Replacement .
The clutch pressure plate cover assembly is faulty | Inspect the clutch pressure plate cover assembly for worn or damaged components. Replace the clutch assembly. Refer to Clutch Assembly Replacement .
Clutch disc splines and input shaft splines worn | Replace the clutch assembly. Refer to Clutch Assembly Replacement . Replace the input shaft. Refer to the transmission manufacturer service manual.