For 1990-2009 cars

### Removal Procedure

1. Insert a narrow-bladed screwdriver into the slot over the wiper blade retainer spring.
2. Pivot the screwdriver so that the blade tip presses downward on the retainer spring and releases the blade from the pin of the wiper arm.
3. Remove the wiper blade from the wiper arm.

### Installation Procedure

Install the wiper blade by snapping it into place on the pin of the wiper arm.