FELT MATERIAL ON I/P TRIM PLATE LOOSE. Chevrolet Celebrity 1989

For 1990-2009 cars

# FELT MATERIAL ON I/P TRIM PLATE LOOSE

#### VEHICLES AFFECTED: 1989 CHEVROLET CELEBRITY

#### Condition:

Owners of some 1989 Chevrolet Celebrities may comment on the felt anti-glare material becoming loose around the edges of the Instrument Panel trim plate.

#### Correction:

1. Remove trim plate.

2. Reattach felt material using 3M Trim Adhesive #08031 or equivalent, following manufacturers instruction.

3. Reinstall trim panel.

Production was changed with the start of the 1990 models.

Use most applicable Labour Operation and Time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.