DRIVE AXLE OIL LEAK THRU VENT REPLACE W/NON VENTED BOOT. Chevrolet Celebrity 1984

For 1990-2009 cars

# DRIVE AXLE OIL LEAK THRU VENT REPLACE W/NON VENTED BOOT

UNDER CONDITIONS OF HEAVY USAGE IN HOT WEATHER, SOME "A AND X" CARS MAY EXHIBIT GREASE LEAKAGE THRU VENT HOLE LOCATED IN THE RIGHT HAND, INNER DRIVE AXLE BOOT. THIS CONDITION CAN BE CORRECTED BY REPLACING THE RIGHT HAND INNER BOOT WITH A NON-VENTED BOOT. PRIOR TO INSTALLING THE NON-VENTED BOOT, THE JOINT SHOULD BE THOROUGHLY CLEANED AND RELUBRICATED WITH THE GREASE INCLUDED IN THE SERVICE KIT. REFER TO APPLICABLE SERVICE MANUAL FOR SERVICE PROCEDURES. TRIPOT HI-TEM SEAL SERVICE KIT P/N 26003940(OR EQUIVALENT). USE APPLICABLE FLAT RATE TIMES.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.