SPARK KNOCK COMMENTS NEW PROM INFORMATION. Chevrolet Celebrity 1984

For 1990-2009 cars

# SPARK KNOCK COMMENTS NEW PROM INFORMATION

#### VEHICLES AFFECTED: 1984 A,F,P & X Series Vehicles Equipped With 2.5L Engines and Automatic Transmissions

A customer comment of spark knock on the 2.5L engine may be received. If normal diagnosis in Section 6E2 of the Service Manual does not repair this condition, a new PROM may be installed, as listed below.

VEHICLE PROM PART NUMBER ------- ---------------- 1984 'A' Car 2.39 axle* 1226910 1984 'A', 'A' Wagon, 'X' with 2.84 axle* 1226997 1984 'X' with 2.39 axle* 1226998 1984 'F' Series 1226911 1984 'P' Series 1226912

*Note: 2.39 transaxle: Code PW transaxle: Code PD

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.