ESCUTCHEON GASKET REPLACEMENT FRONT DOOR LOCK. Chevrolet Celebrity 1985

For 1990-2009 cars

# ESCUTCHEON GASKET REPLACEMENT FRONT DOOR LOCK

A CONDITION HAS BEEN ENCOUNTERED WHERE THE REMOTE HANDLE ESCUTCHEON GASKET MAY GROW OR CREEP FROM BEHIND THE DOOR REMOTE HANDLE AND SWITCH ESCUTCHEON. CARS BUILT ON OR AFTER 10A WILL NOT HAVE THE GASKET INSTALLED. IF A GASKET IS NEEDED, IT MAY BE FABRICATED AND INSTALLED ON THE ESCUTCHEON USING 3M-06375 SCOTCHMOUNT FOAM TAPE OR EQUIVALENT AS SHOWN IN FIGURE 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.