REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY. Chevrolet Celebrity 1985

For 1990-2009 cars

# REWORK OF REAR COMPARTMENT LID HINGE ASSEMBLY

#### MODEL AND YEAR: 1982-1987 CELEBRITY TWO DOOR (A19, A27) WITH REAR SEAT SHOULDER BELTS

Replacement of a rear compartment lid hinge on a vehicle equipped with rear seat shoulder belts may require modifying the hinge.

This modification is to cut a notch in the outboard flange of the replacement part hinge assembly as shown in the illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.