GLOVE BOX DOOR WARPED OR IMPROPER FIT-REPLACEMENT P/N. Chevrolet Celebrity 1985

For 1990-2009 cars

# GLOVE BOX DOOR WARPED OR IMPROPER FIT-REPLACEMENT P/N

GLOVE BOX DOOR WARPED PREVENTING FLUSH FIT

#### VEHICLES AFFECTED: 1985/87 CHEVROLET "A" ------------------ Some 1985/87 Chevrolet "A" cars may have a glove box door that does not fit flush, when closed due to warpage.

If adjustment of the door does not repair the condition (Product-Service Bulletin 86-2-133 dated April 28/86) replace the door assembly with a new one available through the Parts Department P/N 10095411, paint to match.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.