VIBRATION CAUSED BY EXCESSIVE WHEEL RUNOUT. Chevrolet Celebrity 1986

For 1990-2009 cars

# VIBRATION CAUSED BY EXCESSIVE WHEEL RUNOUT

#### VEHICLES AFFECTED: 1985-86 OLDSMOBILE CIERRA WITH STYLED STEEL WHEELS OPTION N67

Some 1985-86 Oldsmobile Cierras may experience a vibration due to excessive wheel lateral runout 1.1 mm (.045" maximum). A new wheel with improved runout specifications, P/N 10067869 is available for this condition.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.